M5 console: m5AlphaAccess @ 0xFFFFFD0200000000

Got Configuration 623

memsize 8000000 pages 4000 

First free page after ROM 0xFFFFFC0000018000

HWRPB 0xFFFFFC0000018000 l1pt 0xFFFFFC0000040000 l2pt 0xFFFFFC0000042000 l3pt_rpb 0xFFFFFC0000044000 l3pt_kernel 0xFFFFFC0000048000 l2reserv 0xFFFFFC0000046000

kstart = 0xFFFFFC0000310000, kend = 0xFFFFFC00008064E8, kentry = 0xFFFFFC0000310000, numCPUs = 0x1

CPU Clock at 2000 MHz IntrClockFrequency=1024 

Booting with 1 processor(s) 

KSP: 0x20043FE8 PTBR 0x20

Console Callback at 0x0, fixup at 0x0, crb offset: 0x510

Memory cluster 0 [0 - 392]

Memory cluster 1 [392 - 15992]

Initalizing mdt_bitmap addr 0xFFFFFC0000038000 mem_pages 4000 

ConsoleDispatch at virt 10000658 phys 18658 val FFFFFC00000100A8

unix_boot_mem ends at FFFFFC0000076000 

k_argc = 0 

jumping to kernel at 0xFFFFFC0000310000, (PCBB 0xFFFFFC0000018180 pfn 1028)

CallbackFixup 0 18000, t7=FFFFFC0000700000

Linux version 2.6.8.1 (binkertn@ziff.eecs.umich.edu) (gcc version 3.4.3) #36 SMP Mon May 2 19:50:53 EDT 2005

Booting GENERIC on Tsunami variation DP264 using machine vector DP264 from SRM

Major Options: SMP LEGACY_START VERBOSE_MCHECK 

Command line: root=/dev/hda1 console=ttyS0

memcluster 0, usage 1, start        0, end      392

memcluster 1, usage 0, start      392, end    16384

freeing pages 1030:16384

reserving pages 1030:1031

SMP: 1 CPUs probed -- cpu_present_mask = 1

Built 1 zonelists

Kernel command line: root=/dev/hda1 console=ttyS0

PID hash table entries: 1024 (order 10: 16384 bytes)

Using epoch = 1900

Console: colour dummy device 80x25

Dentry cache hash table entries: 32768 (order: 5, 262144 bytes)

Inode-cache hash table entries: 16384 (order: 4, 131072 bytes)

Memory: 119072k/131072k available (3058k kernel code, 8680k reserved, 695k data, 480k init)

Mount-cache hash table entries: 512 (order: 0, 8192 bytes)

per-CPU timeslice cutoff: 374.49 usecs.

task migration cache decay timeout: 0 msecs.

SMP mode deactivated.

Brought up 1 CPUs

SMP: Total of 1 processors activated (4002.20 BogoMIPS).

NET: Registered protocol family 16

EISA bus registered

pci: enabling save/restore of SRM state

SCSI subsystem initialized

srm_env: version 0.0.5 loaded successfully

Installing knfsd (copyright (C) 1996 okir@monad.swb.de).

Initializing Cryptographic API

rtc: Standard PC (1900) epoch (1900) detected

Real Time Clock Driver v1.12

Serial: 8250/16550 driver $Revision: 1.90 $ 5 ports, IRQ sharing disabled

ttyS0 at I/O 0x3f8 (irq = 4) is a 8250

loop: loaded (max 8 devices)

Using anticipatory io scheduler

nbd: registered device at major 43

sinic.c: M5 Simple Integrated NIC driver

ns83820.c: National Semiconductor DP83820 10/100/1000 driver.

eth0: ns83820.c: 0x22c: 00000000, subsystem: 0000:0000

eth0: enabling optical transceiver

eth0: ns83820 v0.20: DP83820 v1.3: 00:90:00:00:00:01 io=0x09000000 irq=30 f=sg

Uniform Multi-Platform E-IDE driver Revision: 7.00alpha2

ide: Assuming 33MHz system bus speed for PIO modes; override with idebus=xx

PIIX4: IDE controller at PCI slot 0000:00:00.0

PIIX4: chipset revision 0

PIIX4: 100% native mode on irq 31

    ide0: BM-DMA at 0x8400-0x8407, BIOS settings: hda:DMA, hdb:DMA

    ide1: BM-DMA at 0x8408-0x840f, BIOS settings: hdc:DMA, hdd:DMA

hda: M5 IDE Disk, ATA DISK drive

hdb: M5 IDE Disk, ATA DISK drive

ide0 at 0x8410-0x8417,0x8422 on irq 31

hda: max request size: 128KiB

hda: 163296 sectors (83 MB), CHS=162/16/63, UDMA(33)

 hda: hda1

hdb: max request size: 128KiB

hdb: 4177920 sectors (2139 MB), CHS=4144/16/63, UDMA(33)

 hdb: unknown partition table

scsi0 : scsi_m5, version 1.73 [20040518], dev_size_mb=8, opts=0x0

  Vendor: Linux     Model: scsi_m5       Li  Rev: 0004

  Type:   Direct-Access                      ANSI SCSI revision: 03

SCSI device sda: 16384 512-byte hdwr sectors (8 MB)

SCSI device sda: drive cache: write back

 sda: unknown partition table

Attached scsi disk sda at scsi0, channel 0, id 0, lun 0

mice: PS/2 mouse device common for all mice

NET: Registered protocol family 2

IP: routing cache hash table of 1024 buckets, 16Kbytes

TCP: Hash tables configured (established 8192 bind 8192)

ip_conntrack version 2.1 (512 buckets, 4096 max) - 440 bytes per conntrack

ip_tables: (C) 2000-2002 Netfilter core team

arp_tables: (C) 2002 David S. Miller

Initializing IPsec netlink socket

NET: Registered protocol family 1

NET: Registered protocol family 17

NET: Registered protocol family 15

Bridge firewalling registered

802.1Q VLAN Support v1.8 Ben Greear <greearb@candelatech.com>

All bugs added by David S. Miller <davem@redhat.com>

VFS: Mounted root (ext2 filesystem) readonly.

Freeing unused kernel memory: 480k freed


init started:  BusyBox v1.00-rc2 (2004.11.18-16:22+0000) multi-call binary

PTXdist-0.7.0 (2004-11-18T11:23:40-0500)

mounting filesystems...
EXT2-fs warning: checktime reached, running e2fsck is recommended

loading script...
