M5 console: m5AlphaAccess @ 0xFFFFFD0200000000

Got Configuration 623

memsize 8000000 pages 4000 

First free page after ROM 0xFFFFFC0000018000

HWRPB 0xFFFFFC0000018000 l1pt 0xFFFFFC0000040000 l2pt 0xFFFFFC0000042000 l3pt_rpb 0xFFFFFC0000044000 l3pt_kernel 0xFFFFFC0000048000 l2reserv 0xFFFFFC0000046000

kstart = 0xFFFFFC0000310000, kend = 0xFFFFFC0000855898, kentry = 0xFFFFFC0000310000, numCPUs = 0x2

CPU Clock at 2000 MHz IntrClockFrequency=1024 

Booting with 2 processor(s) 

KSP: 0x20043FE8 PTBR 0x20

KSP: 0x20043FE8 PTBR 0x20

Console Callback at 0x0, fixup at 0x0, crb offset: 0x790

Memory cluster 0 [0 - 392]

Memory cluster 1 [392 - 15992]

Initalizing mdt_bitmap addr 0xFFFFFC0000038000 mem_pages 4000 

ConsoleDispatch at virt 100008D8 phys 188D8 val FFFFFC00000100A8

Bootstraping CPU 1 with sp=0xFFFFFC0000076000

unix_boot_mem ends at FFFFFC0000078000 

k_argc = 0 

jumping to kernel at 0xFFFFFC0000310000, (PCBB 0xFFFFFC0000018180 pfn 1067)

CallbackFixup 0 18000, t7=FFFFFC000070C000

Entering slaveloop for cpu 1 my_rpb=FFFFFC0000018400

Linux version 2.6.13 (hsul@zed.eecs.umich.edu) (gcc version 3.4.3) #1 SMP Sun Oct 8 19:52:07 EDT 2006

Booting GENERIC on Tsunami variation DP264 using machine vector DP264 from SRM

Major Options: SMP LEGACY_START VERBOSE_MCHECK 

Command line: root=/dev/hda1 console=ttyS0

memcluster 0, usage 1, start        0, end      392

memcluster 1, usage 0, start      392, end    16384

freeing pages 1069:16384

reserving pages 1069:1070

4096K Bcache detected; load hit latency 32 cycles, load miss latency 115 cycles

SMP: 2 CPUs probed -- cpu_present_mask = 3

Built 1 zonelists

Kernel command line: root=/dev/hda1 console=ttyS0

PID hash table entries: 1024 (order: 10, 32768 bytes)

Using epoch = 1900

Console: colour dummy device 80x25

Dentry cache hash table entries: 32768 (order: 5, 262144 bytes)

Inode-cache hash table entries: 16384 (order: 4, 131072 bytes)

Memory: 118784k/131072k available (3314k kernel code, 8952k reserved, 983k data, 224k init)

Mount-cache hash table entries: 512

SMP starting up secondaries.

Slave CPU 1 console command START
SlaveCmd: restart FFFFFC0000310020 FFFFFC0000310020 vptb FFFFFFFE00000000 my_rpb FFFFFC0000018400 my_rpb_phys 18400

Brought up 2 CPUs

SMP: Total of 2 processors activated (8000.15 BogoMIPS).

NET: Registered protocol family 16

EISA bus registered

pci: enabling save/restore of SRM state

SCSI subsystem initialized

srm_env: version 0.0.5 loaded successfully

Installing knfsd (copyright (C) 1996 okir@monad.swb.de).

Initializing Cryptographic API

rtc: Standard PC (1900) epoch (1900) detected

Real Time Clock Driver v1.12

Serial: 8250/16550 driver $Revision: 1.90 $ 1 ports, IRQ sharing disabled

ttyS0 at I/O 0x3f8 (irq = 4) is a 8250

io scheduler noop registered

io scheduler anticipatory registered

io scheduler deadline registered

io scheduler cfq registered

loop: loaded (max 8 devices)

nbd: registered device at major 43

ns83820.c: National Semiconductor DP83820 10/100/1000 driver.

PCI: Setting latency timer of device 0000:00:01.0 to 64

eth0: ns83820.c: 0x22c: 00000000, subsystem: 0000:0000

eth0: enabling optical transceiver

eth0: using 64 bit addressing.

eth0: ns83820 v0.22: DP83820 v1.3: 00:90:00:00:00:01 io=0x09000000 irq=30 f=h,sg

tun: Universal TUN/TAP device driver, 1.6

tun: (C) 1999-2004 Max Krasnyansky <maxk@qualcomm.com>

Uniform Multi-Platform E-IDE driver Revision: 7.00alpha2

ide: Assuming 33MHz system bus speed for PIO modes; override with idebus=xx

PIIX4: IDE controller at PCI slot 0000:00:00.0

PIIX4: chipset revision 0

PIIX4: 100% native mode on irq 31

PCI: Setting latency timer of device 0000:00:00.0 to 64

    ide0: BM-DMA at 0x8400-0x8407, BIOS settings: hda:DMA, hdb:DMA

    ide1: BM-DMA at 0x8408-0x840f, BIOS settings: hdc:DMA, hdd:DMA

hda: M5 IDE Disk, ATA DISK drive

hdb: M5 IDE Disk, ATA DISK drive

ide0 at 0x8410-0x8417,0x8422 on irq 31

hda: max request size: 128KiB

hda: 101808 sectors (52 MB), CHS=101/16/63, UDMA(33)

hda: cache flushes not supported

 hda: hda1

hdb: max request size: 128KiB

hdb: 4177920 sectors (2139 MB), CHS=4144/16/63, UDMA(33)

hdb: cache flushes not supported

 hdb: unknown partition table

mice: PS/2 mouse device common for all mice

NET: Registered protocol family 2

IP route cache hash table entries: 4096 (order: 2, 32768 bytes)

TCP established hash table entries: 16384 (order: 5, 262144 bytes)

TCP bind hash table entries: 16384 (order: 5, 262144 bytes)

TCP: Hash tables configured (established 16384 bind 16384)

TCP reno registered

ip_conntrack version 2.1 (512 buckets, 4096 max) - 296 bytes per conntrack

ip_tables: (C) 2000-2002 Netfilter core team

arp_tables: (C) 2002 David S. Miller

TCP bic registered

Initializing IPsec netlink socket

NET: Registered protocol family 1

NET: Registered protocol family 17

NET: Registered protocol family 15

Bridge firewalling registered

802.1Q VLAN Support v1.8 Ben Greear <greearb@candelatech.com>

All bugs added by David S. Miller <davem@redhat.com>

VFS: Mounted root (ext2 filesystem) readonly.

Freeing unused kernel memory: 224k freed


init started:  BusyBox v1.1.0 (2007.03.04-01:07+0000) multi-call binary
mounting filesystems...
EXT2-fs warning: checktime reached, running e2fsck is recommended

loading script...
