// -*- mode:c++ -*-

// Copyright (c) 2010 ARM Limited
// All rights reserved
//
// The license below extends only to copyright in the software and shall
// not be construed as granting a license to any other intellectual
// property including but not limited to intellectual property relating
// to a hardware implementation of the functionality of the software
// licensed hereunder.  You may use the software subject to the license
// terms below provided that you ensure that this notice is replicated
// unmodified and in its entirety in all distributions of the software,
// modified or unmodified, in source code or in binary form.
//
// Copyright (c) 2007-2008 The Florida State University
// All rights reserved.
//
// Redistribution and use in source and binary forms, with or without
// modification, are permitted provided that the following conditions are
// met: redistributions of source code must retain the above copyright
// notice, this list of conditions and the following disclaimer;
// redistributions in binary form must reproduce the above copyright
// notice, this list of conditions and the following disclaimer in the
// documentation and/or other materials provided with the distribution;
// neither the name of the copyright holders nor the names of its
// contributors may be used to endorse or promote products derived from
// this software without specific prior written permission.
//
// THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS
// "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT
// LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR
// A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT
// OWNER OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL,
// SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT
// LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE,
// DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY
// THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
// (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE
// OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
//
// Authors: Stephen Hines

////////////////////////////////////////////////////////////////////
//
// Floating Point operate instructions
//

output header {{

    template<template <typename T> class Base>
    StaticInstPtr
    newNeonMemInst(const unsigned size,
                   const ExtMachInst &machInst,
                   const RegIndex dest, const RegIndex ra,
                   const uint32_t imm, const unsigned extraMemFlags)
    {
        switch (size) {
          case 0:
            return new Base<uint8_t>(machInst, dest, ra, imm, extraMemFlags);
          case 1:
            return new Base<uint16_t>(machInst, dest, ra, imm, extraMemFlags);
          case 2:
            return new Base<uint32_t>(machInst, dest, ra, imm, extraMemFlags);
          case 3:
            return new Base<uint64_t>(machInst, dest, ra, imm, extraMemFlags);
          default:
            panic("Unrecognized width %d for Neon mem inst.\n", (1 << size));
        }
    }

    template<template <typename T> class Base>
    StaticInstPtr
    newNeonMixInst(const unsigned size,
                   const ExtMachInst &machInst,
                   const RegIndex dest, const RegIndex op1,
                   const uint32_t step)
    {
        switch (size) {
          case 0:
            return new Base<uint8_t>(machInst, dest, op1, step);
          case 1:
            return new Base<uint16_t>(machInst, dest, op1, step);
          case 2:
            return new Base<uint32_t>(machInst, dest, op1, step);
          case 3:
            return new Base<uint64_t>(machInst, dest, op1, step);
          default:
            panic("Unrecognized width %d for Neon mem inst.\n", (1 << size));
        }
    }

}};

let {{
    header_output = '''
    StaticInstPtr
    decodeNeonMem(ExtMachInst machInst);

    StaticInstPtr
    decodeNeonData(ExtMachInst machInst);
    '''

    decoder_output = '''
    StaticInstPtr
    decodeNeonMem(ExtMachInst machInst)
    {
        const uint32_t b = bits(machInst, 11, 8);
        const bool single = bits(machInst, 23);
        const bool singleAll = single && (bits(b, 3, 2) == 3);
        const bool load = bits(machInst, 21);

        unsigned width = 0;

        if (single) {
            width = bits(b, 1, 0) + 1;
        } else {
            switch (bits(b, 3, 1)) {
              case 0x0: width = 4;
                break;
              case 0x1: width = (b & 0x1) ? 2 : 1;
                break;
              case 0x2: width = 3;
                break;
              case 0x3: width = 1;
                break;
              case 0x4: width = 2;
                break;
              case 0x5:
                if ((b & 0x1) == 0) {
                    width = 1;
                    break;
                }
                // Fall through on purpose.
              default:
                return new Unknown(machInst);
            }
        }
        assert(width > 0 && width <= 4);

        const RegIndex rm = (RegIndex)(uint32_t)bits(machInst, 3, 0);
        const RegIndex rn = (RegIndex)(uint32_t)bits(machInst, 19, 16);
        const RegIndex vd = (RegIndex)(uint32_t)(bits(machInst, 15, 12) |
                                                 bits(machInst, 22) << 4);
        const uint32_t type = bits(machInst, 11, 8);
        uint32_t size = 0;
        uint32_t align = TLB::MustBeOne;
        unsigned inc = 1;
        unsigned regs = 1;
        unsigned lane = 0;
        if (single) {
            if (singleAll) {
                size = bits(machInst, 7, 6);
                bool t = bits(machInst, 5);
                unsigned eBytes = (1 << size);
                align = (eBytes - 1) | TLB::AllowUnaligned;
                if (width == 1) {
                    regs = t ? 2 : 1;
                    inc = 1;
                } else {
                    regs = width;
                    inc = t ? 2 : 1;
                }
                switch (width) {
                  case 1:
                  case 2:
                    if (bits(machInst, 4))
                        align = width * eBytes - 1;
                    break;
                  case 3:
                    break;
                  case 4:
                    if (size == 3) {
                        if (bits(machInst, 4) == 0)
                            return new Unknown(machInst);
                        size = 2;
                        align = 0xf;
                    } else if (size == 2) {
                        if (bits(machInst, 4))
                            align = 7;
                    } else {
                        if (bits(machInst, 4))
                            align = 4 * eBytes - 1;
                    }
                    break;
                }
            } else {
                size = bits(machInst, 11, 10);
                unsigned eBytes = (1 << size);
                align = (eBytes - 1) | TLB::AllowUnaligned;
                regs = width;
                unsigned indexAlign = bits(machInst, 7, 4);
                // If width is 1, inc is always 1. That's overridden later.
                switch (size) {
                  case 0:
                    inc = 1;
                    lane = bits(indexAlign, 3, 1);
                    break;
                  case 1:
                    inc = bits(indexAlign, 1) ? 2 : 1;
                    lane = bits(indexAlign, 3, 2);
                    break;
                  case 2:
                    inc = bits(indexAlign, 2) ? 2 : 1;
                    lane = bits(indexAlign, 3);
                    break;
                }
                // Override inc for width of 1.
                if (width == 1) {
                    inc = 1;
                }
                switch (width) {
                  case 1:
                    switch (size) {
                      case 0:
                        break;
                      case 1:
                        if (bits(indexAlign, 0))
                            align = 1;
                        break;
                      case 2:
                        if (bits(indexAlign, 1, 0))
                            align = 3;
                        break;
                    }
                    break;
                  case 2:
                    if (bits(indexAlign, 0))
                        align = (2 * eBytes) - 1;
                    break;
                  case 3:
                    break;
                  case 4:
                    switch (size) {
                      case 0:
                      case 1:
                        if (bits(indexAlign, 0))
                            align = (4 * eBytes) - 1;
                        break;
                      case 2:
                        if (bits(indexAlign, 0))
                            align = (4 << bits(indexAlign, 1, 0)) - 1;
                        break;
                    }
                    break;
                }
            }
            if (size == 0x3) {
                return new Unknown(machInst);
            }
        } else {
            size = bits(machInst, 7, 6);
            align = bits(machInst, 5, 4);
            if (align == 0) {
                // @align wasn't specified, so alignment can be turned off.
                align = ((1 << size) - 1) | TLB::AllowUnaligned;
            } else {
                align = ((4 << align) - 1);
            }
            switch (width) {
              case 1:
                switch (type) {
                  case 0x7: regs = 1;
                    break;
                  case 0xa: regs = 2;
                    break;
                  case 0x6: regs = 3;
                    break;
                  case 0x2: regs = 4;
                    break;
                  default:
                    return new Unknown(machInst);
                }
                break;
              case 2:
                // Regs doesn't behave exactly as it does in the manual
                // because they loop over regs registers twice and we break
                // it down in the macroop.
                switch (type) {
                  case 0x8: regs = 2; inc = 1;
                    break;
                  case 0x9: regs = 2; inc = 2;
                    break;
                  case 0x3: regs = 4; inc = 2;
                    break;
                  default:
                    return new Unknown(machInst);
                }
                break;
              case 3:
                regs = 3;
                switch (type) {
                  case 0x4: inc = 1;
                    break;
                  case 0x5: inc = 2;;
                    break;
                  default:
                    return new Unknown(machInst);
                }
                break;
              case 4:
                regs = 4;
                switch (type) {
                  case 0: inc = 1;
                    break;
                  case 1: inc = 2;
                    break;
                  default:
                    return new Unknown(machInst);
                }
                break;
            }
        }

        if (load) {
            // Load instructions.
            if (single) {
                return new VldSingle(machInst, singleAll, width, rn, vd,
                                     regs, inc, size, align, rm, lane);
            } else {
                return new VldMult(machInst, width, rn, vd,
                                   regs, inc, size, align, rm);
            }
        } else {
            // Store instructions.
            if (single) {
                if (singleAll) {
                    return new Unknown(machInst);
                } else {
                    return new VstSingle(machInst, false, width, rn, vd,
                                         regs, inc, size, align, rm, lane);
                }
            } else {
                return new VstMult(machInst, width, rn, vd,
                                   regs, inc, size, align, rm);
            }
        }
        return new Unknown(machInst);
    }
    '''

    decoder_output += '''
    static StaticInstPtr
    decodeNeonThreeRegistersSameLength(ExtMachInst machInst)
    {
        const bool u = THUMB ? bits(machInst, 28) : bits(machInst, 24);
        const uint32_t a = bits(machInst, 11, 8);
        const bool b = bits(machInst, 4);
        const uint32_t c = bits(machInst, 21, 20);
        const IntRegIndex vd =
            (IntRegIndex)(2 * (bits(machInst, 15, 12) |
                               (bits(machInst, 22) << 4)));
        const IntRegIndex vn =
            (IntRegIndex)(2 * (bits(machInst, 19, 16) |
                               (bits(machInst, 7) << 4)));
        const IntRegIndex vm =
            (IntRegIndex)(2 * (bits(machInst, 3, 0) |
                               (bits(machInst, 5) << 4)));
        const unsigned size = bits(machInst, 21, 20);
        const bool q = bits(machInst, 6);
        if (q && ((vd & 0x1) || (vn & 0x1) || (vm & 0x1)))
            return new Unknown(machInst);
        switch (a) {
          case 0x0:
            if (b) {
                if (u) {
                    return decodeNeonUThreeReg<VqaddUD, VqaddUQ>(
                            q, size, machInst, vd, vn, vm);
                } else {
                    return decodeNeonSThreeReg<VqaddSD, VqaddSQ>(
                            q, size, machInst, vd, vn, vm);
                }
            } else {
                if (size == 3)
                    return new Unknown(machInst);
                return decodeNeonUSThreeReg<VhaddD, VhaddQ>(
                        q, u, size, machInst, vd, vn, vm);
            }
          case 0x1:
            if (!b) {
                return decodeNeonUSThreeReg<VrhaddD, VrhaddQ>(
                        q, u, size, machInst, vd, vn, vm);
            } else {
                if (u) {
                    switch (c) {
                      case 0:
                        if (q) {
                            return new VeorQ<uint64_t>(machInst, vd, vn, vm);
                        } else {
                            return new VeorD<uint64_t>(machInst, vd, vn, vm);
                        }
                      case 1:
                        if (q) {
                            return new VbslQ<uint64_t>(machInst, vd, vn, vm);
                        } else {
                            return new VbslD<uint64_t>(machInst, vd, vn, vm);
                        }
                      case 2:
                        if (q) {
                            return new VbitQ<uint64_t>(machInst, vd, vn, vm);
                        } else {
                            return new VbitD<uint64_t>(machInst, vd, vn, vm);
                        }
                      case 3:
                        if (q) {
                            return new VbifQ<uint64_t>(machInst, vd, vn, vm);
                        } else {
                            return new VbifD<uint64_t>(machInst, vd, vn, vm);
                        }
                    }
                } else {
                    switch (c) {
                      case 0:
                        if (q) {
                            return new VandQ<uint64_t>(machInst, vd, vn, vm);
                        } else {
                            return new VandD<uint64_t>(machInst, vd, vn, vm);
                        }
                      case 1:
                        if (q) {
                            return new VbicQ<uint64_t>(machInst, vd, vn, vm);
                        } else {
                            return new VbicD<uint64_t>(machInst, vd, vn, vm);
                        }
                      case 2:
                        if (vn == vm) {
                            if (q) {
                                return new VmovQ<uint64_t>(
                                        machInst, vd, vn, vm);
                            } else {
                                return new VmovD<uint64_t>(
                                        machInst, vd, vn, vm);
                            }
                        } else {
                            if (q) {
                                return new VorrQ<uint64_t>(
                                        machInst, vd, vn, vm);
                            } else {
                                return new VorrD<uint64_t>(
                                        machInst, vd, vn, vm);
                            }
                        }
                      case 3:
                        if (q) {
                            return new VornQ<uint64_t>(
                                    machInst, vd, vn, vm);
                        } else {
                            return new VornD<uint64_t>(
                                    machInst, vd, vn, vm);
                        }
                    }
                }
            }
          case 0x2:
            if (b) {
                if (u) {
                    return decodeNeonUThreeReg<VqsubUD, VqsubUQ>(
                            q, size, machInst, vd, vn, vm);
                } else {
                    return decodeNeonSThreeReg<VqsubSD, VqsubSQ>(
                            q, size, machInst, vd, vn, vm);
                }
            } else {
                if (size == 3)
                    return new Unknown(machInst);
                return decodeNeonUSThreeReg<VhsubD, VhsubQ>(
                        q, u, size, machInst, vd, vn, vm);
            }
          case 0x3:
            if (b) {
                return decodeNeonUSThreeReg<VcgeD, VcgeQ>(
                        q, u, size, machInst, vd, vn, vm);
            } else {
                return decodeNeonUSThreeReg<VcgtD, VcgtQ>(
                        q, u, size, machInst, vd, vn, vm);
            }
          case 0x4:
            if (b) {
                if (u) {
                    return decodeNeonUThreeReg<VqshlUD, VqshlUQ>(
                            q, size, machInst, vd, vm, vn);
                } else {
                    return decodeNeonSThreeReg<VqshlSD, VqshlSQ>(
                            q, size, machInst, vd, vm, vn);
                }
            } else {
                return decodeNeonUSThreeReg<VshlD, VshlQ>(
                        q, u, size, machInst, vd, vm, vn);
            }
          case 0x5:
            if (b) {
                if (u) {
                    return decodeNeonUThreeReg<VqrshlUD, VqrshlUQ>(
                            q, size, machInst, vd, vm, vn);
                } else {
                    return decodeNeonSThreeReg<VqrshlSD, VqrshlSQ>(
                            q, size, machInst, vd, vm, vn);
                }
            } else {
                return decodeNeonUSThreeReg<VrshlD, VrshlQ>(
                        q, u, size, machInst, vd, vm, vn);
            }
          case 0x6:
            if (b) {
                return decodeNeonUSThreeReg<VminD, VminQ>(
                        q, u, size, machInst, vd, vn, vm);
            } else {
                return decodeNeonUSThreeReg<VmaxD, VmaxQ>(
                        q, u, size, machInst, vd, vn, vm);
            }
          case 0x7:
            if (b) {
                return decodeNeonUSThreeReg<VabaD, VabaQ>(
                        q, u, size, machInst, vd, vn, vm);
            } else {
                if (bits(machInst, 23) == 1) {
                    if (q) {
                        return new Unknown(machInst);
                    } else {
                        return decodeNeonUSThreeUSReg<Vabdl>(
                                u, size, machInst, vd, vn, vm);
                    }
                } else {
                    return decodeNeonUSThreeReg<VabdD, VabdQ>(
                            q, u, size, machInst, vd, vn, vm);
                }
            }
          case 0x8:
            if (b) {
                if (u) {
                    return decodeNeonUThreeReg<VceqD, VceqQ>(
                            q, size, machInst, vd, vn, vm);
                } else {
                    return decodeNeonUThreeReg<VtstD, VtstQ>(
                            q, size, machInst, vd, vn, vm);
                }
            } else {
                if (u) {
                    return decodeNeonUThreeReg<NVsubD, NVsubQ>(
                            q, size, machInst, vd, vn, vm);
                } else {
                    return decodeNeonUThreeReg<NVaddD, NVaddQ>(
                            q, size, machInst, vd, vn, vm);
                }
            }
          case 0x9:
            if (b) {
                if (u) {
                    return decodeNeonUThreeReg<NVmulpD, NVmulpQ>(
                            q, size, machInst, vd, vn, vm);
                } else {
                    return decodeNeonSThreeReg<NVmulD, NVmulQ>(
                            q, size, machInst, vd, vn, vm);
                }
            } else {
                if (u) {
                    return decodeNeonUSThreeReg<NVmlsD, NVmlsQ>(
                            q, u, size, machInst, vd, vn, vm);
                } else {
                    return decodeNeonUSThreeReg<NVmlaD, NVmlaQ>(
                            q, u, size, machInst, vd, vn, vm);
                }
            }
          case 0xa:
            if (b) {
                return decodeNeonUSThreeReg<VpminD, VpminQ>(
                        q, u, size, machInst, vd, vn, vm);
            } else {
                return decodeNeonUSThreeReg<VpmaxD, VpmaxQ>(
                        q, u, size, machInst, vd, vn, vm);
            }
          case 0xb:
            if (b) {
                if (u) {
                    return new Unknown(machInst);
                } else {
                    return decodeNeonUThreeReg<NVpaddD, NVpaddQ>(
                            q, size, machInst, vd, vn, vm);
                }
            } else {
                if (u) {
                    return decodeNeonSThreeSReg<VqrdmulhD, VqrdmulhQ>(
                            q, size, machInst, vd, vn, vm);
                } else {
                    return decodeNeonSThreeSReg<VqdmulhD, VqdmulhQ>(
                            q, size, machInst, vd, vn, vm);
                }
            }
          case 0xc:
            return new Unknown(machInst);
          case 0xd:
            if (b) {
                if (u) {
                    if (bits(c, 1) == 0) {
                        if (q) {
                            return new NVmulQFp<float>(machInst, vd, vn, vm);
                        } else {
                            return new NVmulDFp<float>(machInst, vd, vn, vm);
                        }
                    } else {
                        return new Unknown(machInst);
                    }
                } else {
                    if (bits(c, 1) == 0) {
                        if (q) {
                            return new NVmlaQFp<float>(machInst, vd, vn, vm);
                        } else {
                            return new NVmlaDFp<float>(machInst, vd, vn, vm);
                        }
                    } else {
                        if (q) {
                            return new NVmlsQFp<float>(machInst, vd, vn, vm);
                        } else {
                            return new NVmlsDFp<float>(machInst, vd, vn, vm);
                        }
                    }
                }
            } else {
                if (u) {
                    if (bits(c, 1) == 0) {
                        if (q) {
                            return new VpaddQFp<float>(machInst, vd, vn, vm);
                        } else {
                            return new VpaddDFp<float>(machInst, vd, vn, vm);
                        }
                    } else {
                        if (q) {
                            return new VabdQFp<float>(machInst, vd, vn, vm);
                        } else {
                            return new VabdDFp<float>(machInst, vd, vn, vm);
                        }
                    }
                } else {
                    if (bits(c, 1) == 0) {
                        if (q) {
                            return new VaddQFp<float>(machInst, vd, vn, vm);
                        } else {
                            return new VaddDFp<float>(machInst, vd, vn, vm);
                        }
                    } else {
                        if (q) {
                            return new VsubQFp<float>(machInst, vd, vn, vm);
                        } else {
                            return new VsubDFp<float>(machInst, vd, vn, vm);
                        }
                    }
                }
            }
          case 0xe:
            if (b) {
                if (u) {
                    if (bits(c, 1) == 0) {
                        if (q) {
                            return new VacgeQFp<float>(machInst, vd, vn, vm);
                        } else {
                            return new VacgeDFp<float>(machInst, vd, vn, vm);
                        }
                    } else {
                        if (q) {
                            return new VacgtQFp<float>(machInst, vd, vn, vm);
                        } else {
                            return new VacgtDFp<float>(machInst, vd, vn, vm);
                        }
                    }
                } else {
                    return new Unknown(machInst);
                }
            } else {
                if (u) {
                    if (bits(c, 1) == 0) {
                        if (q) {
                            return new VcgeQFp<float>(machInst, vd, vn, vm);
                        } else {
                            return new VcgeDFp<float>(machInst, vd, vn, vm);
                        }
                    } else {
                        if (q) {
                            return new VcgtQFp<float>(machInst, vd, vn, vm);
                        } else {
                            return new VcgtDFp<float>(machInst, vd, vn, vm);
                        }
                    }
                } else {
                    if (bits(c, 1) == 0) {
                        if (q) {
                            return new VceqQFp<float>(machInst, vd, vn, vm);
                        } else {
                            return new VceqDFp<float>(machInst, vd, vn, vm);
                        }
                    } else {
                        return new Unknown(machInst);
                    }
                }
            }
          case 0xf:
            if (b) {
                if (u) {
                    return new Unknown(machInst);
                } else {
                    if (bits(c, 1) == 0) {
                        if (q) {
                            return new VrecpsQFp<float>(machInst, vd, vn, vm);
                        } else {
                            return new VrecpsDFp<float>(machInst, vd, vn, vm);
                        }
                    } else {
                        if (q) {
                            return new VrsqrtsQFp<float>(machInst, vd, vn, vm);
                        } else {
                            return new VrsqrtsDFp<float>(machInst, vd, vn, vm);
                        }
                    }
                }
            } else {
                if (u) {
                    if (bits(c, 1) == 0) {
                        if (q) {
                            return new VpmaxQFp<float>(machInst, vd, vn, vm);
                        } else {
                            return new VpmaxDFp<float>(machInst, vd, vn, vm);
                        }
                    } else {
                        if (q) {
                            return new VpminQFp<float>(machInst, vd, vn, vm);
                        } else {
                            return new VpminDFp<float>(machInst, vd, vn, vm);
                        }
                    }
                } else {
                    if (bits(c, 1) == 0) {
                        if (q) {
                            return new VmaxQFp<float>(machInst, vd, vn, vm);
                        } else {
                            return new VmaxDFp<float>(machInst, vd, vn, vm);
                        }
                    } else {
                        if (q) {
                            return new VminQFp<float>(machInst, vd, vn, vm);
                        } else {
                            return new VminDFp<float>(machInst, vd, vn, vm);
                        }
                    }
                }
            }
        }
        return new Unknown(machInst);
    }

    static StaticInstPtr
    decodeNeonOneRegModImm(ExtMachInst machInst)
    {
        const IntRegIndex vd =
            (IntRegIndex)(2 * (bits(machInst, 15, 12) |
                               (bits(machInst, 22) << 4)));
        const bool q = bits(machInst, 6);
        const bool op = bits(machInst, 5);
        const uint8_t cmode = bits(machInst, 11, 8);
        const uint8_t imm = ((THUMB ? bits(machInst, 28) :
                                      bits(machInst, 24)) << 7) |
                            (bits(machInst, 18, 16) << 4) |
                            (bits(machInst, 3, 0) << 0);

        // Check for invalid immediate encodings and return an unknown op
        // if it happens
        bool immValid = true;
        const uint64_t bigImm = simd_modified_imm(op, cmode, imm, immValid);
        if (!immValid) {
            return new Unknown(machInst);
        }

        if (op) {
            if (bits(cmode, 3) == 0) {
                if (bits(cmode, 0) == 0) {
                    if (q)
                        return new NVmvniQ<uint64_t>(machInst, vd, bigImm);
                    else
                        return new NVmvniD<uint64_t>(machInst, vd, bigImm);
                } else {
                    if (q)
                        return new NVbiciQ<uint64_t>(machInst, vd, bigImm);
                    else
                        return new NVbiciD<uint64_t>(machInst, vd, bigImm);
                }
            } else {
                if (bits(cmode, 2) == 1) {
                    switch (bits(cmode, 1, 0)) {
                      case 0:
                      case 1:
                        if (q)
                            return new NVmvniQ<uint64_t>(machInst, vd, bigImm);
                        else
                            return new NVmvniD<uint64_t>(machInst, vd, bigImm);
                      case 2:
                        if (q)
                            return new NVmoviQ<uint64_t>(machInst, vd, bigImm);
                        else
                            return new NVmoviD<uint64_t>(machInst, vd, bigImm);
                      case 3:
                        if (q)
                            return new Unknown(machInst);
                        else
                            return new Unknown(machInst);
                    }
                } else {
                    if (bits(cmode, 0) == 0) {
                        if (q)
                            return new NVmvniQ<uint64_t>(machInst, vd, bigImm);
                        else
                            return new NVmvniD<uint64_t>(machInst, vd, bigImm);
                    } else {
                        if (q)
                            return new NVbiciQ<uint64_t>(machInst, vd, bigImm);
                        else
                            return new NVbiciD<uint64_t>(machInst, vd, bigImm);
                    }
                }
            }
        } else {
            if (bits(cmode, 3) == 0) {
                if (bits(cmode, 0) == 0) {
                    if (q)
                        return new NVmoviQ<uint64_t>(machInst, vd, bigImm);
                    else
                        return new NVmoviD<uint64_t>(machInst, vd, bigImm);
                } else {
                    if (q)
                        return new NVorriQ<uint64_t>(machInst, vd, bigImm);
                    else
                        return new NVorriD<uint64_t>(machInst, vd, bigImm);
                }
            } else {
                if (bits(cmode, 2) == 1) {
                    if (q)
                        return new NVmoviQ<uint64_t>(machInst, vd, bigImm);
                    else
                        return new NVmoviD<uint64_t>(machInst, vd, bigImm);
                } else {
                    if (bits(cmode, 0) == 0) {
                        if (q)
                            return new NVmoviQ<uint64_t>(machInst, vd, bigImm);
                        else
                            return new NVmoviD<uint64_t>(machInst, vd, bigImm);
                    } else {
                        if (q)
                            return new NVorriQ<uint64_t>(machInst, vd, bigImm);
                        else
                            return new NVorriD<uint64_t>(machInst, vd, bigImm);
                    }
                }
            }
        }
        return new Unknown(machInst);
    }

    static StaticInstPtr
    decodeNeonTwoRegAndShift(ExtMachInst machInst)
    {
        const uint32_t a = bits(machInst, 11, 8);
        const bool u = THUMB ? bits(machInst, 28) : bits(machInst, 24);
        const bool b = bits(machInst, 6);
        const bool l = bits(machInst, 7);
        const IntRegIndex vd =
            (IntRegIndex)(2 * (bits(machInst, 15, 12) |
                               (bits(machInst, 22) << 4)));
        const IntRegIndex vm =
            (IntRegIndex)(2 * (bits(machInst, 3, 0) |
                               (bits(machInst, 5) << 4)));
        unsigned imm6 = bits(machInst, 21, 16);
        unsigned imm = ((l ? 1 : 0) << 6) | imm6;
        unsigned size = 3;
        unsigned lShiftAmt = 0;
        unsigned bitSel;
        for (bitSel = 1 << 6; true; bitSel >>= 1) {
            if (bitSel & imm)
                break;
            else if (!size)
                return new Unknown(machInst);
            size--;
        }
        lShiftAmt = imm6 & ~bitSel;
        unsigned rShiftAmt = 0;
        if (a != 0xe && a != 0xf) {
            if (size > 2)
                rShiftAmt = 64 - imm6;
            else
                rShiftAmt = 2 * (8 << size) - imm6;
        }

        switch (a) {
          case 0x0:
            return decodeNeonUSTwoShiftReg<NVshrD, NVshrQ>(
                    b, u, size, machInst, vd, vm, rShiftAmt);
          case 0x1:
            return decodeNeonUSTwoShiftReg<NVsraD, NVsraQ>(
                    b, u, size, machInst, vd, vm, rShiftAmt);
          case 0x2:
            return decodeNeonUSTwoShiftReg<NVrshrD, NVrshrQ>(
                    b, u, size, machInst, vd, vm, rShiftAmt);
          case 0x3:
            return decodeNeonUSTwoShiftReg<NVrsraD, NVrsraQ>(
                    b, u, size, machInst, vd, vm, rShiftAmt);
          case 0x4:
            if (u) {
                return decodeNeonUTwoShiftReg<NVsriD, NVsriQ>(
                        b, size, machInst, vd, vm, rShiftAmt);
            } else {
                return new Unknown(machInst);
            }
          case 0x5:
            if (u) {
                return decodeNeonUTwoShiftReg<NVsliD, NVsliQ>(
                        b, size, machInst, vd, vm, lShiftAmt);
            } else {
                return decodeNeonUTwoShiftReg<NVshlD, NVshlQ>(
                        b, size, machInst, vd, vm, lShiftAmt);
            }
          case 0x6:
          case 0x7:
            if (u) {
                if (a == 0x6) {
                    return decodeNeonSTwoShiftReg<NVqshlusD, NVqshlusQ>(
                            b, size, machInst, vd, vm, lShiftAmt);
                } else {
                    return decodeNeonUTwoShiftReg<NVqshluD, NVqshluQ>(
                            b, size, machInst, vd, vm, lShiftAmt);
                }
            } else {
                return decodeNeonSTwoShiftReg<NVqshlD, NVqshlQ>(
                        b, size, machInst, vd, vm, lShiftAmt);
            }
          case 0x8:
            if (l) {
                return new Unknown(machInst);
            } else if (u) {
                return decodeNeonSTwoShiftSReg<NVqshruns, NVqrshruns>(
                        b, size, machInst, vd, vm, rShiftAmt);
            } else {
                return decodeNeonUTwoShiftSReg<NVshrn, NVrshrn>(
                        b, size, machInst, vd, vm, rShiftAmt);
            }
          case 0x9:
            if (l) {
                return new Unknown(machInst);
            } else if (u) {
                return decodeNeonUTwoShiftSReg<NVqshrun, NVqrshrun>(
                        b, size, machInst, vd, vm, rShiftAmt);
            } else {
                return decodeNeonSTwoShiftSReg<NVqshrn, NVqrshrn>(
                        b, size, machInst, vd, vm, rShiftAmt);
            }
          case 0xa:
            if (l || b) {
                return new Unknown(machInst);
            } else {
                return decodeNeonUSTwoShiftSReg<NVmovl, NVshll>(
                        lShiftAmt, u, size, machInst, vd, vm, lShiftAmt);
            }
          case 0xe:
            if (l) {
                return new Unknown(machInst);
            } else {
                if (bits(imm6, 5) == 0)
                    return new Unknown(machInst);
                if (u) {
                    if (b) {
                        return new NVcvtu2fpQ<float>(
                                machInst, vd, vm, 64 - imm6);
                    } else {
                        return new NVcvtu2fpD<float>(
                                machInst, vd, vm, 64 - imm6);
                    }
                } else {
                    if (b) {
                        return new NVcvts2fpQ<float>(
                                machInst, vd, vm, 64 - imm6);
                    } else {
                        return new NVcvts2fpD<float>(
                                machInst, vd, vm, 64 - imm6);
                    }
                }
            }
          case 0xf:
            if (l) {
                return new Unknown(machInst);
            } else {
                if (bits(imm6, 5) == 0)
                    return new Unknown(machInst);
                if (u) {
                    if (b) {
                        return new NVcvt2ufxQ<float>(
                                machInst, vd, vm, 64 - imm6);
                    } else {
                        return new NVcvt2ufxD<float>(
                                machInst, vd, vm, 64 - imm6);
                    }
                } else {
                    if (b) {
                        return new NVcvt2sfxQ<float>(
                                machInst, vd, vm, 64 - imm6);
                    } else {
                        return new NVcvt2sfxD<float>(
                                machInst, vd, vm, 64 - imm6);
                    }
                }
            }
        }
        return new Unknown(machInst);
    }

    static StaticInstPtr
    decodeNeonThreeRegDiffLengths(ExtMachInst machInst)
    {
        const bool u = THUMB ? bits(machInst, 28) : bits(machInst, 24);
        const uint32_t a = bits(machInst, 11, 8);
        const IntRegIndex vd =
            (IntRegIndex)(2 * (bits(machInst, 15, 12) |
                               (bits(machInst, 22) << 4)));
        const IntRegIndex vn =
            (IntRegIndex)(2 * (bits(machInst, 19, 16) |
                               (bits(machInst, 7) << 4)));
        const IntRegIndex vm =
            (IntRegIndex)(2 * (bits(machInst, 3, 0) |
                               (bits(machInst, 5) << 4)));
        const unsigned size = bits(machInst, 21, 20);
        switch (a) {
          case 0x0:
            return decodeNeonUSThreeUSReg<Vaddl>(
                    u, size, machInst, vd, vn, vm);
          case 0x1:
            return decodeNeonUSThreeUSReg<Vaddw>(
                    u, size, machInst, vd, vn, vm);
          case 0x2:
            return decodeNeonUSThreeUSReg<Vsubl>(
                    u, size, machInst, vd, vn, vm);
          case 0x3:
            return decodeNeonUSThreeUSReg<Vsubw>(
                    u, size, machInst, vd, vn, vm);
          case 0x4:
            if (u) {
                return decodeNeonUThreeUSReg<Vraddhn>(
                        size, machInst, vd, vn, vm);
            } else {
                return decodeNeonUThreeUSReg<Vaddhn>(
                        size, machInst, vd, vn, vm);
            }
          case 0x5:
            return decodeNeonUSThreeUSReg<Vabal>(
                    u, size, machInst, vd, vn, vm);
          case 0x6:
            if (u) {
                return decodeNeonUThreeUSReg<Vrsubhn>(
                        size, machInst, vd, vn, vm);
            } else {
                return decodeNeonUThreeUSReg<Vsubhn>(
                        size, machInst, vd, vn, vm);
            }
          case 0x7:
            if (bits(machInst, 23)) {
                return decodeNeonUSThreeUSReg<Vabdl>(
                        u, size, machInst, vd, vn, vm);
            } else {
                return decodeNeonUSThreeReg<VabdD, VabdQ>(
                        bits(machInst, 6), u, size, machInst, vd, vn, vm);
            }
          case 0x8:
            return decodeNeonUSThreeUSReg<Vmlal>(
                    u, size, machInst, vd, vn, vm);
          case 0xa:
            return decodeNeonUSThreeUSReg<Vmlsl>(
                    u, size, machInst, vd, vn, vm);
          case 0x9:
            if (u) {
                return new Unknown(machInst);
            } else {
                return decodeNeonSThreeUSReg<Vqdmlal>(
                        size, machInst, vd, vn, vm);
            }
          case 0xb:
            if (u) {
                return new Unknown(machInst);
            } else {
                return decodeNeonSThreeUSReg<Vqdmlsl>(
                        size, machInst, vd, vn, vm);
            }
          case 0xc:
            return decodeNeonUSThreeUSReg<Vmull>(
                    u, size, machInst, vd, vn, vm);
          case 0xd:
            if (u) {
                return new Unknown(machInst);
            } else {
                return decodeNeonSThreeUSReg<Vqdmull>(
                        size, machInst, vd, vn, vm);
            }
          case 0xe:
            return decodeNeonUThreeUSReg<Vmullp>(
                    size, machInst, vd, vn, vm);
        }
        return new Unknown(machInst);
    }

    static StaticInstPtr
    decodeNeonTwoRegScalar(ExtMachInst machInst)
    {
        const bool u = THUMB ? bits(machInst, 28) : bits(machInst, 24);
        const uint32_t a = bits(machInst, 11, 8);
        const unsigned size = bits(machInst, 21, 20);
        const IntRegIndex vd =
            (IntRegIndex)(2 * (bits(machInst, 15, 12) |
                               (bits(machInst, 22) << 4)));
        const IntRegIndex vn =
            (IntRegIndex)(2 * (bits(machInst, 19, 16) |
                               (bits(machInst, 7) << 4)));
        const IntRegIndex vm = (size == 2) ?
            (IntRegIndex)(2 * bits(machInst, 3, 0)) :
            (IntRegIndex)(2 * bits(machInst, 2, 0));
        const unsigned index = (size == 2) ? (unsigned)bits(machInst, 5) :
            (bits(machInst, 3) | (bits(machInst, 5) << 1));
        switch (a) {
          case 0x0:
            if (u) {
                switch (size) {
                  case 1:
                    return new VmlasQ<uint16_t>(machInst, vd, vn, vm, index);
                  case 2:
                    return new VmlasQ<uint32_t>(machInst, vd, vn, vm, index);
                  default:
                    return new Unknown(machInst);
                }
            } else {
                switch (size) {
                  case 1:
                    return new VmlasD<uint16_t>(machInst, vd, vn, vm, index);
                  case 2:
                    return new VmlasD<uint32_t>(machInst, vd, vn, vm, index);
                  default:
                    return new Unknown(machInst);
                }
            }
          case 0x1:
            if (u)
                return new VmlasQFp<float>(machInst, vd, vn, vm, index);
            else
                return new VmlasDFp<float>(machInst, vd, vn, vm, index);
          case 0x4:
            if (u) {
                switch (size) {
                  case 1:
                    return new VmlssQ<uint16_t>(machInst, vd, vn, vm, index);
                  case 2:
                    return new VmlssQ<uint32_t>(machInst, vd, vn, vm, index);
                  default:
                    return new Unknown(machInst);
                }
            } else {
                switch (size) {
                  case 1:
                    return new VmlssD<uint16_t>(machInst, vd, vn, vm, index);
                  case 2:
                    return new VmlssD<uint32_t>(machInst, vd, vn, vm, index);
                  default:
                    return new Unknown(machInst);
                }
            }
          case 0x5:
            if (u)
                return new VmlssQFp<float>(machInst, vd, vn, vm, index);
            else
                return new VmlssDFp<float>(machInst, vd, vn, vm, index);
          case 0x2:
            if (u) {
                switch (size) {
                  case 1:
                    return new Vmlals<uint16_t>(machInst, vd, vn, vm, index);
                  case 2:
                    return new Vmlals<uint32_t>(machInst, vd, vn, vm, index);
                  default:
                    return new Unknown(machInst);
                }
            } else {
                switch (size) {
                  case 1:
                    return new Vmlals<int16_t>(machInst, vd, vn, vm, index);
                  case 2:
                    return new Vmlals<int32_t>(machInst, vd, vn, vm, index);
                  default:
                    return new Unknown(machInst);
                }
            }
          case 0x6:
            if (u) {
                switch (size) {
                  case 1:
                    return new Vmlsls<uint16_t>(machInst, vd, vn, vm, index);
                  case 2:
                    return new Vmlsls<uint32_t>(machInst, vd, vn, vm, index);
                  default:
                    return new Unknown(machInst);
                }
            } else {
                switch (size) {
                  case 1:
                    return new Vmlsls<int16_t>(machInst, vd, vn, vm, index);
                  case 2:
                    return new Vmlsls<int32_t>(machInst, vd, vn, vm, index);
                  default:
                    return new Unknown(machInst);
                }
            }
          case 0x3:
            if (u) {
                return new Unknown(machInst);
            } else {
                switch (size) {
                  case 1:
                    return new Vqdmlals<int16_t>(machInst, vd, vn, vm, index);
                  case 2:
                    return new Vqdmlals<int32_t>(machInst, vd, vn, vm, index);
                  default:
                    return new Unknown(machInst);
                }
            }
          case 0x7:
            if (u) {
                return new Unknown(machInst);
            } else {
                switch (size) {
                  case 1:
                    return new Vqdmlsls<int16_t>(machInst, vd, vn, vm, index);
                  case 2:
                    return new Vqdmlsls<int32_t>(machInst, vd, vn, vm, index);
                  default:
                    return new Unknown(machInst);
                }
            }
          case 0x8:
            if (u) {
                switch (size) {
                  case 1:
                    return new VmulsQ<uint16_t>(machInst, vd, vn, vm, index);
                  case 2:
                    return new VmulsQ<uint32_t>(machInst, vd, vn, vm, index);
                  default:
                    return new Unknown(machInst);
                }
            } else {
                switch (size) {
                  case 1:
                    return new VmulsD<uint16_t>(machInst, vd, vn, vm, index);
                  case 2:
                    return new VmulsD<uint32_t>(machInst, vd, vn, vm, index);
                  default:
                    return new Unknown(machInst);
                }
            }
          case 0x9:
            if (u)
                return new VmulsQFp<float>(machInst, vd, vn, vm, index);
            else
                return new VmulsDFp<float>(machInst, vd, vn, vm, index);
          case 0xa:
            if (u) {
                switch (size) {
                  case 1:
                    return new Vmulls<uint16_t>(machInst, vd, vn, vm, index);
                  case 2:
                    return new Vmulls<uint32_t>(machInst, vd, vn, vm, index);
                  default:
                    return new Unknown(machInst);
                }
            } else {
                switch (size) {
                  case 1:
                    return new Vmulls<int16_t>(machInst, vd, vn, vm, index);
                  case 2:
                    return new Vmulls<int32_t>(machInst, vd, vn, vm, index);
                  default:
                    return new Unknown(machInst);
                }
            }
          case 0xb:
            if (u) {
                return new Unknown(machInst);
            } else {
                if (u) {
                    switch (size) {
                      case 1:
                        return new Vqdmulls<uint16_t>(
                                machInst, vd, vn, vm, index);
                      case 2:
                        return new Vqdmulls<uint32_t>(
                                machInst, vd, vn, vm, index);
                      default:
                        return new Unknown(machInst);
                    }
                } else {
                    switch (size) {
                      case 1:
                        return new Vqdmulls<int16_t>(
                                machInst, vd, vn, vm, index);
                      case 2:
                        return new Vqdmulls<int32_t>(
                                machInst, vd, vn, vm, index);
                      default:
                        return new Unknown(machInst);
                    }
                }
            }
          case 0xc:
            if (u) {
                switch (size) {
                  case 1:
                    return new VqdmulhsQ<int16_t>(
                            machInst, vd, vn, vm, index);
                  case 2:
                    return new VqdmulhsQ<int32_t>(
                            machInst, vd, vn, vm, index);
                  default:
                    return new Unknown(machInst);
                }
            } else {
                switch (size) {
                  case 1:
                    return new VqdmulhsD<int16_t>(
                            machInst, vd, vn, vm, index);
                  case 2:
                    return new VqdmulhsD<int32_t>(
                            machInst, vd, vn, vm, index);
                  default:
                    return new Unknown(machInst);
                }
            }
          case 0xd:
            if (u) {
                switch (size) {
                  case 1:
                    return new VqrdmulhsQ<int16_t>(
                            machInst, vd, vn, vm, index);
                  case 2:
                    return new VqrdmulhsQ<int32_t>(
                            machInst, vd, vn, vm, index);
                  default:
                    return new Unknown(machInst);
                }
            } else {
                switch (size) {
                  case 1:
                    return new VqrdmulhsD<int16_t>(
                            machInst, vd, vn, vm, index);
                  case 2:
                    return new VqrdmulhsD<int32_t>(
                            machInst, vd, vn, vm, index);
                  default:
                    return new Unknown(machInst);
                }
            }
        }
        return new Unknown(machInst);
    }

    static StaticInstPtr
    decodeNeonTwoRegMisc(ExtMachInst machInst)
    {
        const uint32_t a = bits(machInst, 17, 16);
        const uint32_t b = bits(machInst, 10, 6);
        const bool q = bits(machInst, 6);
        const IntRegIndex vd =
            (IntRegIndex)(2 * (bits(machInst, 15, 12) |
                               (bits(machInst, 22) << 4)));
        const IntRegIndex vm =
            (IntRegIndex)(2 * (bits(machInst, 3, 0) |
                               (bits(machInst, 5) << 4)));
        const unsigned size = bits(machInst, 19, 18);
        switch (a) {
          case 0x0:
            switch (bits(b, 4, 1)) {
              case 0x0:
                switch (size) {
                  case 0:
                    if (q) {
                        return new NVrev64Q<uint8_t>(machInst, vd, vm);
                    } else {
                        return new NVrev64D<uint8_t>(machInst, vd, vm);
                    }
                  case 1:
                    if (q) {
                        return new NVrev64Q<uint16_t>(machInst, vd, vm);
                    } else {
                        return new NVrev64D<uint16_t>(machInst, vd, vm);
                    }
                  case 2:
                    if (q) {
                        return new NVrev64Q<uint32_t>(machInst, vd, vm);
                    } else {
                        return new NVrev64D<uint32_t>(machInst, vd, vm);
                    }
                  default:
                    return new Unknown(machInst);
                }
              case 0x1:
                switch (size) {
                  case 0:
                    if (q) {
                        return new NVrev32Q<uint8_t>(machInst, vd, vm);
                    } else {
                        return new NVrev32D<uint8_t>(machInst, vd, vm);
                    }
                  case 1:
                    if (q) {
                        return new NVrev32Q<uint16_t>(machInst, vd, vm);
                    } else {
                        return new NVrev32D<uint16_t>(machInst, vd, vm);
                    }
                  default:
                    return new Unknown(machInst);
                }
              case 0x2:
                if (size != 0) {
                    return new Unknown(machInst);
                } else if (q) {
                    return new NVrev16Q<uint8_t>(machInst, vd, vm);
                } else {
                    return new NVrev16D<uint8_t>(machInst, vd, vm);
                }
              case 0x4:
                return decodeNeonSTwoMiscSReg<NVpaddlD, NVpaddlQ>(
                        q, size, machInst, vd, vm);
              case 0x5:
                return decodeNeonUTwoMiscSReg<NVpaddlD, NVpaddlQ>(
                        q, size, machInst, vd, vm);
              case 0x8:
                return decodeNeonSTwoMiscReg<NVclsD, NVclsQ>(
                        q, size, machInst, vd, vm);
              case 0x9:
                return decodeNeonSTwoMiscReg<NVclzD, NVclzQ>(
                        q, size, machInst, vd, vm);
              case 0xa:
                return decodeNeonUTwoMiscReg<NVcntD, NVcntQ>(
                        q, size, machInst, vd, vm);
              case 0xb:
                if (q)
                    return new NVmvnQ<uint64_t>(machInst, vd, vm);
                else
                    return new NVmvnD<uint64_t>(machInst, vd, vm);
              case 0xc:
                return decodeNeonSTwoMiscSReg<NVpadalD, NVpadalQ>(
                        q, size, machInst, vd, vm);
              case 0xd:
                return decodeNeonUTwoMiscSReg<NVpadalD, NVpadalQ>(
                        q, size, machInst, vd, vm);
              case 0xe:
                return decodeNeonSTwoMiscReg<NVqabsD, NVqabsQ>(
                        q, size, machInst, vd, vm);
              case 0xf:
                return decodeNeonSTwoMiscReg<NVqnegD, NVqnegQ>(
                        q, size, machInst, vd, vm);
              default:
                return new Unknown(machInst);
            }
          case 0x1:
            switch (bits(b, 3, 1)) {
              case 0x0:
                if (bits(b, 4)) {
                    if (q) {
                        return new NVcgtQFp<float>(machInst, vd, vm);
                    } else {
                        return new NVcgtDFp<float>(machInst, vd, vm);
                    }
                } else {
                    return decodeNeonSTwoMiscReg<NVcgtD, NVcgtQ>(
                            q, size, machInst, vd, vm);
                }
              case 0x1:
                if (bits(b, 4)) {
                    if (q) {
                        return new NVcgeQFp<float>(machInst, vd, vm);
                    } else {
                        return new NVcgeDFp<float>(machInst, vd, vm);
                    }
                } else {
                    return decodeNeonSTwoMiscReg<NVcgeD, NVcgeQ>(
                            q, size, machInst, vd, vm);
                }
              case 0x2:
                if (bits(b, 4)) {
                    if (q) {
                        return new NVceqQFp<float>(machInst, vd, vm);
                    } else {
                        return new NVceqDFp<float>(machInst, vd, vm);
                    }
                } else {
                    return decodeNeonSTwoMiscReg<NVceqD, NVceqQ>(
                            q, size, machInst, vd, vm);
                }
              case 0x3:
                if (bits(b, 4)) {
                    if (q) {
                        return new NVcleQFp<float>(machInst, vd, vm);
                    } else {
                        return new NVcleDFp<float>(machInst, vd, vm);
                    }
                } else {
                    return decodeNeonSTwoMiscReg<NVcleD, NVcleQ>(
                            q, size, machInst, vd, vm);
                }
              case 0x4:
                if (bits(b, 4)) {
                    if (q) {
                        return new NVcltQFp<float>(machInst, vd, vm);
                    } else {
                        return new NVcltDFp<float>(machInst, vd, vm);
                    }
                } else {
                    return decodeNeonSTwoMiscReg<NVcltD, NVcltQ>(
                            q, size, machInst, vd, vm);
                }
              case 0x6:
                if (bits(machInst, 10)) {
                    if (q)
                        return new NVabsQFp<float>(machInst, vd, vm);
                    else
                        return new NVabsDFp<float>(machInst, vd, vm);
                } else {
                    return decodeNeonSTwoMiscReg<NVabsD, NVabsQ>(
                            q, size, machInst, vd, vm);
                }
              case 0x7:
                if (bits(machInst, 10)) {
                    if (q)
                        return new NVnegQFp<float>(machInst, vd, vm);
                    else
                        return new NVnegDFp<float>(machInst, vd, vm);
                } else {
                    return decodeNeonSTwoMiscReg<NVnegD, NVnegQ>(
                            q, size, machInst, vd, vm);
                }
            }
          case 0x2:
            switch (bits(b, 4, 1)) {
              case 0x0:
                if (q)
                    return new NVswpQ<uint64_t>(machInst, vd, vm);
                else
                    return new NVswpD<uint64_t>(machInst, vd, vm);
              case 0x1:
                return decodeNeonUTwoMiscReg<NVtrnD, NVtrnQ>(
                        q, size, machInst, vd, vm);
              case 0x2:
                return decodeNeonUTwoMiscReg<NVuzpD, NVuzpQ>(
                        q, size, machInst, vd, vm);
              case 0x3:
                return decodeNeonUTwoMiscReg<NVzipD, NVzipQ>(
                        q, size, machInst, vd, vm);
              case 0x4:
                if (b == 0x8) {
                    return decodeNeonUTwoMiscUSReg<NVmovn>(
                            size, machInst, vd, vm);
                } else {
                    return decodeNeonSTwoMiscUSReg<NVqmovuns>(
                            size, machInst, vd, vm);
                }
              case 0x5:
                if (q) {
                    return decodeNeonUTwoMiscUSReg<NVqmovun>(
                            size, machInst, vd, vm);
                } else {
                    return decodeNeonSTwoMiscUSReg<NVqmovn>(
                            size, machInst, vd, vm);
                }
              case 0x6:
                if (b == 0xc) {
                    const IntRegIndex vd =
                        (IntRegIndex)(2 * (bits(machInst, 15, 12) |
                                           (bits(machInst, 22) << 4)));
                    const IntRegIndex vm =
                        (IntRegIndex)(2 * (bits(machInst, 3, 0) |
                                           (bits(machInst, 5) << 4)));
                    unsigned size = bits(machInst, 19, 18);
                    return decodeNeonSTwoShiftUSReg<NVshll>(
                            size, machInst, vd, vm, 8 << size);
                } else {
                    return new Unknown(machInst);
                }
              case 0xc:
              case 0xe:
                if (b == 0x18) {
                    if (size != 1 || (vm % 2))
                        return new Unknown(machInst);
                    return new NVcvts2h<uint16_t>(machInst, vd, vm);
                } else if (b == 0x1c) {
                    if (size != 1 || (vd % 2))
                        return new Unknown(machInst);
                    return new NVcvth2s<uint16_t>(machInst, vd, vm);
                } else {
                    return new Unknown(machInst);
                }
              default:
                return new Unknown(machInst);
            }
          case 0x3:
            if (bits(b, 4, 3) == 0x3) {
                if ((q && (vd % 2 || vm % 2)) || size != 2) {
                    return new Unknown(machInst);
                } else {
                    if (bits(b, 2)) {
                        if (bits(b, 1)) {
                            if (q) {
                                return new NVcvt2ufxQ<float>(
                                        machInst, vd, vm, 0);
                            } else {
                                return new NVcvt2ufxD<float>(
                                        machInst, vd, vm, 0);
                            }
                        } else {
                            if (q) {
                                return new NVcvt2sfxQ<float>(
                                        machInst, vd, vm, 0);
                            } else {
                                return new NVcvt2sfxD<float>(
                                        machInst, vd, vm, 0);
                            }
                        }
                    } else {
                        if (bits(b, 1)) {
                            if (q) {
                                return new NVcvtu2fpQ<float>(
                                        machInst, vd, vm, 0);
                            } else {
                                return new NVcvtu2fpD<float>(
                                        machInst, vd, vm, 0);
                            }
                        } else {
                            if (q) {
                                return new NVcvts2fpQ<float>(
                                        machInst, vd, vm, 0);
                            } else {
                                return new NVcvts2fpD<float>(
                                        machInst, vd, vm, 0);
                            }
                        }
                    }
                }
            } else if ((b & 0x1a) == 0x10) {
                if (bits(b, 2)) {
                    if (q) {
                        return new NVrecpeQFp<float>(machInst, vd, vm);
                    } else {
                        return new NVrecpeDFp<float>(machInst, vd, vm);
                    }
                } else {
                    if (q) {
                        return new NVrecpeQ<uint32_t>(machInst, vd, vm);
                    } else {
                        return new NVrecpeD<uint32_t>(machInst, vd, vm);
                    }
                }
            } else if ((b & 0x1a) == 0x12) {
                if (bits(b, 2)) {
                    if (q) {
                        return new NVrsqrteQFp<float>(machInst, vd, vm);
                    } else {
                        return new NVrsqrteDFp<float>(machInst, vd, vm);
                    }
                } else {
                    if (q) {
                        return new NVrsqrteQ<uint32_t>(machInst, vd, vm);
                    } else {
                        return new NVrsqrteD<uint32_t>(machInst, vd, vm);
                    }
                }
            } else {
                return new Unknown(machInst);
            }
        }
        return new Unknown(machInst);
    }

    StaticInstPtr
    decodeNeonData(ExtMachInst machInst)
    {
        const bool u = THUMB ? bits(machInst, 28) : bits(machInst, 24);
        const uint32_t a = bits(machInst, 23, 19);
        const uint32_t b = bits(machInst, 11, 8);
        const uint32_t c = bits(machInst, 7, 4);
        if (bits(a, 4) == 0) {
            return decodeNeonThreeRegistersSameLength(machInst);
        } else if ((c & 0x9) == 1) {
            if ((a & 0x7) == 0) {
                return decodeNeonOneRegModImm(machInst);
            } else {
                return decodeNeonTwoRegAndShift(machInst);
            }
        } else if ((c & 0x9) == 9) {
            return decodeNeonTwoRegAndShift(machInst);
        } else if (bits(a, 2, 1) != 0x3) {
            if ((c & 0x5) == 0) {
                return decodeNeonThreeRegDiffLengths(machInst);
            } else if ((c & 0x5) == 4) {
                return decodeNeonTwoRegScalar(machInst);
            }
        } else if ((a & 0x16) == 0x16) {
            const IntRegIndex vd =
                (IntRegIndex)(2 * (bits(machInst, 15, 12) |
                                   (bits(machInst, 22) << 4)));
            const IntRegIndex vn =
                (IntRegIndex)(2 * (bits(machInst, 19, 16) |
                                   (bits(machInst, 7) << 4)));
            const IntRegIndex vm =
                (IntRegIndex)(2 * (bits(machInst, 3, 0) |
                                   (bits(machInst, 5) << 4)));
            if (!u) {
                if (bits(c, 0) == 0) {
                    unsigned imm4 = bits(machInst, 11, 8);
                    bool q = bits(machInst, 6);
                    if (imm4 >= 16 && !q)
                        return new Unknown(machInst);
                    if (q) {
                        return new NVextQ<uint8_t>(machInst, vd, vn, vm, imm4);
                    } else {
                        return new NVextD<uint8_t>(machInst, vd, vn, vm, imm4);
                    }
                }
            } else if (bits(b, 3) == 0 && bits(c, 0) == 0) {
                return decodeNeonTwoRegMisc(machInst);
            } else if (bits(b, 3, 2) == 0x2 && bits(c, 0) == 0) {
                unsigned length = bits(machInst, 9, 8) + 1;
                if ((uint32_t)vn / 2 + length > 32)
                    return new Unknown(machInst);
                if (bits(machInst, 6) == 0) {
                    switch (length) {
                      case 1:
                        return new NVtbl1(machInst, vd, vn, vm);
                      case 2:
                        return new NVtbl2(machInst, vd, vn, vm);
                      case 3:
                        return new NVtbl3(machInst, vd, vn, vm);
                      case 4:
                        return new NVtbl4(machInst, vd, vn, vm);
                    }
                } else {
                    switch (length) {
                      case 1:
                        return new NVtbx1(machInst, vd, vn, vm);
                      case 2:
                        return new NVtbx2(machInst, vd, vn, vm);
                      case 3:
                        return new NVtbx3(machInst, vd, vn, vm);
                      case 4:
                        return new NVtbx4(machInst, vd, vn, vm);
                    }
                }
            } else if (b == 0xc && (c & 0x9) == 0) {
                unsigned imm4 = bits(machInst, 19, 16);
                if (bits(imm4, 2, 0) == 0)
                    return new Unknown(machInst);
                unsigned size = 0;
                while ((imm4 & 0x1) == 0) {
                    size++;
                    imm4 >>= 1;
                }
                unsigned index = imm4 >> 1;
                const bool q = bits(machInst, 6);
                return decodeNeonUTwoShiftSReg<NVdupD, NVdupQ>(
                        q, size, machInst, vd, vm, index);
            }
        }
        return new Unknown(machInst);
    }
    '''
}};

def format ThumbNeonMem() {{
    decode_block = '''
    return decodeNeonMem(machInst);
    '''
}};

def format ThumbNeonData() {{
    decode_block = '''
    return decodeNeonData(machInst);
    '''
}};

let {{
    header_output = '''
    StaticInstPtr
    decodeExtensionRegLoadStore(ExtMachInst machInst);
    '''
    decoder_output = '''
    StaticInstPtr
    decodeExtensionRegLoadStore(ExtMachInst machInst)
    {
        const uint32_t opcode = bits(machInst, 24, 20);
        const uint32_t offset = bits(machInst, 7, 0);
        const bool single = (bits(machInst, 8) == 0);
        const IntRegIndex rn = (IntRegIndex)(uint32_t)bits(machInst, 19, 16);
        RegIndex vd;
        if (single) {
            vd = (RegIndex)(uint32_t)((bits(machInst, 15, 12) << 1) |
                                      bits(machInst, 22));
        } else {
            vd = (RegIndex)(uint32_t)((bits(machInst, 15, 12) << 1) |
                                      (bits(machInst, 22) << 5));
        }
        switch (bits(opcode, 4, 3)) {
          case 0x0:
            if (bits(opcode, 4, 1) == 0x2 &&
                    !(machInst.thumb == 1 && bits(machInst, 28) == 1) &&
                    !(machInst.thumb == 0 && machInst.condCode == 0xf)) {
                if ((bits(machInst, 7, 4) & 0xd) != 1) {
                    break;
                }
                const IntRegIndex rt =
                    (IntRegIndex)(uint32_t)bits(machInst, 15, 12);
                const IntRegIndex rt2 =
                    (IntRegIndex)(uint32_t)bits(machInst, 19, 16);
                const bool op = bits(machInst, 20);
                uint32_t vm;
                if (single) {
                    vm = (bits(machInst, 3, 0) << 1) | bits(machInst, 5);
                } else {
                    vm = (bits(machInst, 3, 0) << 1) |
                         (bits(machInst, 5) << 5);
                }
                if (op) {
                    return new Vmov2Core2Reg(machInst, rt, rt2,
                                             (IntRegIndex)vm);
                } else {
                    return new Vmov2Reg2Core(machInst, (IntRegIndex)vm,
                                             rt, rt2);
                }
            }
            break;
          case 0x1:
            {
                if (offset == 0 || vd + offset/2 > NumFloatArchRegs) {
                    break;
                }
                switch (bits(opcode, 1, 0)) {
                  case 0x0:
                    return new VLdmStm(machInst, rn, vd, single,
                                       true, false, false, offset);
                  case 0x1:
                    return new VLdmStm(machInst, rn, vd, single,
                                       true, false, true, offset);
                  case 0x2:
                    return new VLdmStm(machInst, rn, vd, single,
                                       true, true, false, offset);
                  case 0x3:
                    // If rn == sp, then this is called vpop.
                    return new VLdmStm(machInst, rn, vd, single,
                                       true, true, true, offset);
                }
            }
          case 0x2:
            if (bits(opcode, 1, 0) == 0x2) {
                // If rn == sp, then this is called vpush.
                return new VLdmStm(machInst, rn, vd, single,
                                   false, true, false, offset);
            } else if (bits(opcode, 1, 0) == 0x3) {
                return new VLdmStm(machInst, rn, vd, single,
                                   false, true, true, offset);
            }
            // Fall through on purpose
          case 0x3:
            const bool up = (bits(machInst, 23) == 1);
            const uint32_t imm = bits(machInst, 7, 0) << 2;
            RegIndex vd;
            if (single) {
                vd = (RegIndex)(uint32_t)((bits(machInst, 15, 12) << 1) |
                                          (bits(machInst, 22)));
            } else {
                vd = (RegIndex)(uint32_t)((bits(machInst, 15, 12) << 1) |
                                          (bits(machInst, 22) << 5));
            }
            if (bits(opcode, 1, 0) == 0x0) {
                if (single) {
                    if (up) {
                        return new %(vstr_us)s(machInst, vd, rn, up, imm);
                    } else {
                        return new %(vstr_s)s(machInst, vd, rn, up, imm);
                    }
                } else {
                    if (up) {
                        return new %(vstr_ud)s(machInst, vd, vd + 1,
                                               rn, up, imm);
                    } else {
                        return new %(vstr_d)s(machInst, vd, vd + 1,
                                              rn, up, imm);
                    }
                }
            } else if (bits(opcode, 1, 0) == 0x1) {
                if (single) {
                    if (up) {
                        return new %(vldr_us)s(machInst, vd, rn, up, imm);
                    } else {
                        return new %(vldr_s)s(machInst, vd, rn, up, imm);
                    }
                } else {
                    if (up) {
                        return new %(vldr_ud)s(machInst, vd, vd + 1,
                                               rn, up, imm);
                    } else {
                        return new %(vldr_d)s(machInst, vd, vd + 1,
                                              rn, up, imm);
                    }
                }
            }
        }
        return new Unknown(machInst);
    }
    ''' % {
        "vldr_us" : "VLDR_" + loadImmClassName(False, True, False),
        "vldr_s" : "VLDR_" + loadImmClassName(False, False, False),
        "vldr_ud" : "VLDR_" + loadDoubleImmClassName(False, True, False),
        "vldr_d" : "VLDR_" + loadDoubleImmClassName(False, False, False),
        "vstr_us" : "VSTR_" + storeImmClassName(False, True, False),
        "vstr_s" : "VSTR_" + storeImmClassName(False, False, False),
        "vstr_ud" : "VSTR_" + storeDoubleImmClassName(False, True, False),
        "vstr_d" : "VSTR_" + storeDoubleImmClassName(False, False, False)
    }
}};

def format ExtensionRegLoadStore() {{
    decode_block = '''
    return decodeExtensionRegLoadStore(machInst);
    '''
}};

let {{
    header_output = '''
    StaticInstPtr
    decodeShortFpTransfer(ExtMachInst machInst);
    '''
    decoder_output = '''
    StaticInstPtr
    decodeShortFpTransfer(ExtMachInst machInst)
    {
        const uint32_t l = bits(machInst, 20);
        const uint32_t c = bits(machInst, 8);
        const uint32_t a = bits(machInst, 23, 21);
        const uint32_t b = bits(machInst, 6, 5);
        if ((machInst.thumb == 1 && bits(machInst, 28) == 1) ||
            (machInst.thumb == 0 && machInst.condCode == 0xf)) {
            return new Unknown(machInst);
        }
        if (l == 0 && c == 0) {
            if (a == 0) {
                const uint32_t vn = (bits(machInst, 19, 16) << 1) |
                                    bits(machInst, 7);
                const IntRegIndex rt =
                    (IntRegIndex)(uint32_t)bits(machInst, 15, 12);
                if (bits(machInst, 20) == 1) {
                    return new VmovRegCoreW(machInst, rt, (IntRegIndex)vn);
                } else {
                    return new VmovCoreRegW(machInst, (IntRegIndex)vn, rt);
                }
            } else if (a == 0x7) {
                const IntRegIndex rt =
                    (IntRegIndex)(uint32_t)bits(machInst, 15, 12);
                uint32_t specReg = bits(machInst, 19, 16);
                switch (specReg) {
                  case 0:
                    specReg = MISCREG_FPSID;
                    break;
                  case 1:
                    specReg = MISCREG_FPSCR;
                    break;
                  case 6:
                    specReg = MISCREG_MVFR1;
                    break;
                  case 7:
                    specReg = MISCREG_MVFR0;
                    break;
                  case 8:
                    specReg = MISCREG_FPEXC;
                    break;
                  default:
                    return new Unknown(machInst);
                }
                if (specReg == MISCREG_FPSCR) {
                    return new VmsrFpscr(machInst, (IntRegIndex)specReg, rt);
                } else {
                    return new Vmsr(machInst, (IntRegIndex)specReg, rt);
                }
            }
        } else if (l == 0 && c == 1) {
            if (bits(a, 2) == 0) {
                uint32_t vd = (bits(machInst, 7) << 5) |
                              (bits(machInst, 19, 16) << 1);
                // Handle accessing each single precision half of the vector.
                vd += bits(machInst, 21);
                const IntRegIndex rt =
                    (IntRegIndex)(uint32_t)bits(machInst, 15, 12);
                if (bits(machInst, 22) == 1) {
                    return new VmovCoreRegB(machInst, (IntRegIndex)vd,
                                            rt, bits(machInst, 6, 5));
                } else if (bits(machInst, 5) == 1) {
                    return new VmovCoreRegH(machInst, (IntRegIndex)vd,
                                            rt, bits(machInst, 6));
                } else if (bits(machInst, 6) == 0) {
                    return new VmovCoreRegW(machInst, (IntRegIndex)vd, rt);
                } else {
                    return new Unknown(machInst);
                }
            } else if (bits(b, 1) == 0) {
                bool q = bits(machInst, 21);
                unsigned be = (bits(machInst, 22) << 1) | (bits(machInst, 5));
                IntRegIndex vd = (IntRegIndex)(2 * (uint32_t)
                    (bits(machInst, 19, 16) | (bits(machInst, 7) << 4)));
                IntRegIndex rt = (IntRegIndex)(uint32_t)
                    bits(machInst, 15, 12);
                if (q) {
                    switch (be) {
                      case 0:
                        return new NVdupQGpr<uint32_t>(machInst, vd, rt);
                      case 1:
                        return new NVdupQGpr<uint16_t>(machInst, vd, rt);
                      case 2:
                        return new NVdupQGpr<uint8_t>(machInst, vd, rt);
                      case 3:
                        return new Unknown(machInst);
                    }
                } else {
                    switch (be) {
                      case 0:
                        return new NVdupDGpr<uint32_t>(machInst, vd, rt);
                      case 1:
                        return new NVdupDGpr<uint16_t>(machInst, vd, rt);
                      case 2:
                        return new NVdupDGpr<uint8_t>(machInst, vd, rt);
                      case 3:
                        return new Unknown(machInst);
                    }
                }
            }
        } else if (l == 1 && c == 0) {
            if (a == 0) {
                const uint32_t vn = (bits(machInst, 19, 16) << 1) |
                                    bits(machInst, 7);
                const IntRegIndex rt =
                    (IntRegIndex)(uint32_t)bits(machInst, 15, 12);
                if (bits(machInst, 20) == 1) {
                    return new VmovRegCoreW(machInst, rt, (IntRegIndex)vn);
                } else {
                    return new VmovCoreRegW(machInst, (IntRegIndex)vn, rt);
                }
            } else if (a == 7) {
                const IntRegIndex rt =
                    (IntRegIndex)(uint32_t)bits(machInst, 15, 12);
                uint32_t specReg = bits(machInst, 19, 16);
                switch (specReg) {
                  case 0:
                    specReg = MISCREG_FPSID;
                    break;
                  case 1:
                    specReg = MISCREG_FPSCR;
                    break;
                  case 6:
                    specReg = MISCREG_MVFR1;
                    break;
                  case 7:
                    specReg = MISCREG_MVFR0;
                    break;
                  case 8:
                    specReg = MISCREG_FPEXC;
                    break;
                  default:
                    return new Unknown(machInst);
                }
                if (rt == 0xf) {
                    CPSR cpsrMask = 0;
                    cpsrMask.n = 1;
                    cpsrMask.z = 1;
                    cpsrMask.c = 1;
                    cpsrMask.v = 1;
                    if (specReg == MISCREG_FPSCR) {
                        return new VmrsApsrFpscr(machInst, INTREG_CONDCODES,
                                (IntRegIndex)specReg, (uint32_t)cpsrMask);
                    } else {
                        return new VmrsApsr(machInst, INTREG_CONDCODES,
                                (IntRegIndex)specReg, (uint32_t)cpsrMask);
                    }
                } else if (specReg == MISCREG_FPSCR) {
                    return new VmrsFpscr(machInst, rt, (IntRegIndex)specReg);
                } else {
                    return new Vmrs(machInst, rt, (IntRegIndex)specReg);
                }
            }
        } else {
            uint32_t vd = (bits(machInst, 7) << 5) |
                          (bits(machInst, 19, 16) << 1);
            // Handle indexing into each single precision half of the vector.
            vd += bits(machInst, 21);
            uint32_t index;
            const IntRegIndex rt =
                (IntRegIndex)(uint32_t)bits(machInst, 15, 12);
            const bool u = (bits(machInst, 23) == 1);
            if (bits(machInst, 22) == 1) {
                index = bits(machInst, 6, 5);
                if (u) {
                    return new VmovRegCoreUB(machInst, rt,
                                             (IntRegIndex)vd, index);
                } else {
                    return new VmovRegCoreSB(machInst, rt,
                                             (IntRegIndex)vd, index);
                }
            } else if (bits(machInst, 5) == 1) {
                index = bits(machInst, 6);
                if (u) {
                    return new VmovRegCoreUH(machInst, rt,
                                             (IntRegIndex)vd, index);
                } else {
                    return new VmovRegCoreSH(machInst, rt,
                                             (IntRegIndex)vd, index);
                }
            } else if (bits(machInst, 6) == 0 && !u) {
                return new VmovRegCoreW(machInst, rt, (IntRegIndex)vd);
            } else {
                return new Unknown(machInst);
            }
        }
        return new Unknown(machInst);
    }
    '''
}};

def format ShortFpTransfer() {{
    decode_block = '''
    return decodeShortFpTransfer(machInst);
    '''
}};

let {{
    header_output = '''
    StaticInstPtr
    decodeVfpData(ExtMachInst machInst);
    '''
    decoder_output = '''
    StaticInstPtr
    decodeVfpData(ExtMachInst machInst)
    {
        const uint32_t opc1 = bits(machInst, 23, 20);
        const uint32_t opc2 = bits(machInst, 19, 16);
        const uint32_t opc3 = bits(machInst, 7, 6);
        //const uint32_t opc4 = bits(machInst, 3, 0);
        const bool single = (bits(machInst, 8) == 0);
        // Used to select between vcmp and vcmpe.
        const bool e = (bits(machInst, 7) == 1);
        IntRegIndex vd;
        IntRegIndex vm;
        IntRegIndex vn;
        if (single) {
            vd = (IntRegIndex)(bits(machInst, 22) |
                    (bits(machInst, 15, 12) << 1));
            vm = (IntRegIndex)(bits(machInst, 5) |
                    (bits(machInst, 3, 0) << 1));
            vn = (IntRegIndex)(bits(machInst, 7) |
                    (bits(machInst, 19, 16) << 1));
        } else {
            vd = (IntRegIndex)((bits(machInst, 22) << 5) |
                    (bits(machInst, 15, 12) << 1));
            vm = (IntRegIndex)((bits(machInst, 5) << 5) |
                    (bits(machInst, 3, 0) << 1));
            vn = (IntRegIndex)((bits(machInst, 7) << 5) |
                    (bits(machInst, 19, 16) << 1));
        }
        switch (opc1 & 0xb /* 1011 */) {
          case 0x0:
            if (bits(machInst, 6) == 0) {
                if (single) {
                    return decodeVfpRegRegRegOp<VmlaS>(
                            machInst, vd, vn, vm, false);
                } else {
                    return decodeVfpRegRegRegOp<VmlaD>(
                            machInst, vd, vn, vm, true);
                }
            } else {
                if (single) {
                    return decodeVfpRegRegRegOp<VmlsS>(
                            machInst, vd, vn, vm, false);
                } else {
                    return decodeVfpRegRegRegOp<VmlsD>(
                            machInst, vd, vn, vm, true);
                }
            }
          case 0x1:
            if (bits(machInst, 6) == 1) {
                if (single) {
                    return decodeVfpRegRegRegOp<VnmlaS>(
                            machInst, vd, vn, vm, false);
                } else {
                    return decodeVfpRegRegRegOp<VnmlaD>(
                            machInst, vd, vn, vm, true);
                }
            } else {
                if (single) {
                    return decodeVfpRegRegRegOp<VnmlsS>(
                            machInst, vd, vn, vm, false);
                } else {
                    return decodeVfpRegRegRegOp<VnmlsD>(
                            machInst, vd, vn, vm, true);
                }
            }
          case 0x2:
            if ((opc3 & 0x1) == 0) {
                if (single) {
                    return decodeVfpRegRegRegOp<VmulS>(
                            machInst, vd, vn, vm, false);
                } else {
                    return decodeVfpRegRegRegOp<VmulD>(
                            machInst, vd, vn, vm, true);
                }
            } else {
                if (single) {
                    return decodeVfpRegRegRegOp<VnmulS>(
                            machInst, vd, vn, vm, false);
                } else {
                    return decodeVfpRegRegRegOp<VnmulD>(
                            machInst, vd, vn, vm, true);
                }
            }
          case 0x3:
            if ((opc3 & 0x1) == 0) {
                if (single) {
                    return decodeVfpRegRegRegOp<VaddS>(
                            machInst, vd, vn, vm, false);
                } else {
                    return decodeVfpRegRegRegOp<VaddD>(
                            machInst, vd, vn, vm, true);
                }
            } else {
                if (single) {
                    return decodeVfpRegRegRegOp<VsubS>(
                            machInst, vd, vn, vm, false);
                } else {
                    return decodeVfpRegRegRegOp<VsubD>(
                            machInst, vd, vn, vm, true);
                }
            }
          case 0x8:
            if ((opc3 & 0x1) == 0) {
                if (single) {
                    return decodeVfpRegRegRegOp<VdivS>(
                            machInst, vd, vn, vm, false);
                } else {
                    return decodeVfpRegRegRegOp<VdivD>(
                            machInst, vd, vn, vm, true);
                }
            }
            break;
          case 0xb:
            if ((opc3 & 0x1) == 0) {
                const uint32_t baseImm =
                    bits(machInst, 3, 0) | (bits(machInst, 19, 16) << 4);
                if (single) {
                    uint32_t imm = vfp_modified_imm(baseImm, false);
                    return decodeVfpRegImmOp<VmovImmS>(
                            machInst, vd, imm, false);
                } else {
                    uint64_t imm = vfp_modified_imm(baseImm, true);
                    return decodeVfpRegImmOp<VmovImmD>(
                            machInst, vd, imm, true);
                }
            }
            switch (opc2) {
              case 0x0:
                if (opc3 == 1) {
                    if (single) {
                        return decodeVfpRegRegOp<VmovRegS>(
                                machInst, vd, vm, false);
                    } else {
                        return decodeVfpRegRegOp<VmovRegD>(
                                machInst, vd, vm, true);
                    }
                } else {
                    if (single) {
                        return decodeVfpRegRegOp<VabsS>(
                                machInst, vd, vm, false);
                    } else {
                        return decodeVfpRegRegOp<VabsD>(
                                machInst, vd, vm, true);
                    }
                }
              case 0x1:
                if (opc3 == 1) {
                    if (single) {
                        return decodeVfpRegRegOp<VnegS>(
                                machInst, vd, vm, false);
                    } else {
                        return decodeVfpRegRegOp<VnegD>(
                                machInst, vd, vm, true);
                    }
                } else {
                    if (single) {
                        return decodeVfpRegRegOp<VsqrtS>(
                                machInst, vd, vm, false);
                    } else {
                        return decodeVfpRegRegOp<VsqrtD>(
                                machInst, vd, vm, true);
                    }
                }
              case 0x2:
              case 0x3:
                {
                    const bool toHalf = bits(machInst, 16);
                    const bool top = bits(machInst, 7);
                    if (top) {
                        if (toHalf) {
                            return new VcvtFpSFpHT(machInst, vd, vm);
                        } else {
                            return new VcvtFpHTFpS(machInst, vd, vm);
                        }
                    } else {
                        if (toHalf) {
                            return new VcvtFpSFpHB(machInst, vd, vm);
                        } else {
                            return new VcvtFpHBFpS(machInst, vd, vm);
                        }
                    }
                }
              case 0x4:
                if (single) {
                    if (e) {
                        return new VcmpeS(machInst, vd, vm);
                    } else {
                        return new VcmpS(machInst, vd, vm);
                    }
                } else {
                    if (e) {
                        return new VcmpeD(machInst, vd, vm);
                    } else {
                        return new VcmpD(machInst, vd, vm);
                    }
                }
              case 0x5:
                if (single) {
                    if (e) {
                        return new VcmpeZeroS(machInst, vd, 0);
                    } else {
                        return new VcmpZeroS(machInst, vd, 0);
                    }
                } else {
                    if (e) {
                        return new VcmpeZeroD(machInst, vd, 0);
                    } else {
                        return new VcmpZeroD(machInst, vd, 0);
                    }
                }
              case 0x7:
                if (opc3 == 0x3) {
                    if (single) {
                        vm = (IntRegIndex)(bits(machInst, 5) |
                                (bits(machInst, 3, 0) << 1));
                        return new VcvtFpSFpD(machInst, vd, vm);
                    } else {
                        vd = (IntRegIndex)(bits(machInst, 22) |
                                (bits(machInst, 15, 12) << 1));
                        return new VcvtFpDFpS(machInst, vd, vm);
                    }
                }
                break;
              case 0x8:
                if (bits(machInst, 7) == 0) {
                    if (single) {
                        return new VcvtUIntFpS(machInst, vd, vm);
                    } else {
                        vm = (IntRegIndex)(bits(machInst, 5) |
                                (bits(machInst, 3, 0) << 1));
                        return new VcvtUIntFpD(machInst, vd, vm);
                    }
                } else {
                    if (single) {
                        return new VcvtSIntFpS(machInst, vd, vm);
                    } else {
                        vm = (IntRegIndex)(bits(machInst, 5) |
                                (bits(machInst, 3, 0) << 1));
                        return new VcvtSIntFpD(machInst, vd, vm);
                    }
                }
              case 0xa:
                {
                    const bool half = (bits(machInst, 7) == 0);
                    const uint32_t imm = bits(machInst, 5) |
                                         (bits(machInst, 3, 0) << 1);
                    const uint32_t size =
                        (bits(machInst, 7) == 0 ? 16 : 32) - imm;
                    if (single) {
                        if (half) {
                            return new VcvtSHFixedFpS(machInst, vd, vd, size);
                        } else {
                            return new VcvtSFixedFpS(machInst, vd, vd, size);
                        }
                    } else {
                        if (half) {
                            return new VcvtSHFixedFpD(machInst, vd, vd, size);
                        } else {
                            return new VcvtSFixedFpD(machInst, vd, vd, size);
                        }
                    }
                }
              case 0xb:
                {
                    const bool half = (bits(machInst, 7) == 0);
                    const uint32_t imm = bits(machInst, 5) |
                                         (bits(machInst, 3, 0) << 1);
                    const uint32_t size =
                        (bits(machInst, 7) == 0 ? 16 : 32) - imm;
                    if (single) {
                        if (half) {
                            return new VcvtUHFixedFpS(machInst, vd, vd, size);
                        } else {
                            return new VcvtUFixedFpS(machInst, vd, vd, size);
                        }
                    } else {
                        if (half) {
                            return new VcvtUHFixedFpD(machInst, vd, vd, size);
                        } else {
                            return new VcvtUFixedFpD(machInst, vd, vd, size);
                        }
                    }
                }
              case 0xc:
                if (bits(machInst, 7) == 0) {
                    if (single) {
                        return new VcvtFpUIntSR(machInst, vd, vm);
                    } else {
                        vd = (IntRegIndex)(bits(machInst, 22) |
                                (bits(machInst, 15, 12) << 1));
                        return new VcvtFpUIntDR(machInst, vd, vm);
                    }
                } else {
                    if (single) {
                        return new VcvtFpUIntS(machInst, vd, vm);
                    } else {
                        vd = (IntRegIndex)(bits(machInst, 22) |
                                (bits(machInst, 15, 12) << 1));
                        return new VcvtFpUIntD(machInst, vd, vm);
                    }
                }
              case 0xd:
                if (bits(machInst, 7) == 0) {
                    if (single) {
                        return new VcvtFpSIntSR(machInst, vd, vm);
                    } else {
                        vd = (IntRegIndex)(bits(machInst, 22) |
                                (bits(machInst, 15, 12) << 1));
                        return new VcvtFpSIntDR(machInst, vd, vm);
                    }
                } else {
                    if (single) {
                        return new VcvtFpSIntS(machInst, vd, vm);
                    } else {
                        vd = (IntRegIndex)(bits(machInst, 22) |
                                (bits(machInst, 15, 12) << 1));
                        return new VcvtFpSIntD(machInst, vd, vm);
                    }
                }
              case 0xe:
                {
                    const bool half = (bits(machInst, 7) == 0);
                    const uint32_t imm = bits(machInst, 5) |
                                         (bits(machInst, 3, 0) << 1);
                    const uint32_t size =
                        (bits(machInst, 7) == 0 ? 16 : 32) - imm;
                    if (single) {
                        if (half) {
                            return new VcvtFpSHFixedS(machInst, vd, vd, size);
                        } else {
                            return new VcvtFpSFixedS(machInst, vd, vd, size);
                        }
                    } else {
                        if (half) {
                            return new VcvtFpSHFixedD(machInst, vd, vd, size);
                        } else {
                            return new VcvtFpSFixedD(machInst, vd, vd, size);
                        }
                    }
                }
              case 0xf:
                {
                    const bool half = (bits(machInst, 7) == 0);
                    const uint32_t imm = bits(machInst, 5) |
                                         (bits(machInst, 3, 0) << 1);
                    const uint32_t size =
                        (bits(machInst, 7) == 0 ? 16 : 32) - imm;
                    if (single) {
                        if (half) {
                            return new VcvtFpUHFixedS(machInst, vd, vd, size);
                        } else {
                            return new VcvtFpUFixedS(machInst, vd, vd, size);
                        }
                    } else {
                        if (half) {
                            return new VcvtFpUHFixedD(machInst, vd, vd, size);
                        } else {
                            return new VcvtFpUFixedD(machInst, vd, vd, size);
                        }
                    }
                }
            }
            break;
        }
        return new Unknown(machInst);
    }
    '''
}};

def format VfpData() {{
    decode_block = '''
    return decodeVfpData(machInst);
    '''
}};
