Linux version 2.6.22.9 (blackga@nacho) (gcc version 4.1.2 (Gentoo 4.1.2)) #2 Mon Oct 8 13:13:00 PDT 2007
Command line: earlyprintk=ttyS0 console=ttyS0 lpj=7999923 root=/dev/hda1
BIOS-provided physical RAM map:
 BIOS-e820: 0000000000000000 - 0000000000100000 (reserved)
 BIOS-e820: 0000000000100000 - 0000000008000000 (usable)
end_pfn_map = 32768
kernel direct mapping tables up to 8000000 @ 100000-102000
DMI 2.5 present.
Zone PFN ranges:
  DMA           256 ->     4096
  DMA32        4096 ->  1048576
  Normal    1048576 ->  1048576
early_node_map[1] active PFN ranges
    0:      256 ->    32768
Intel MultiProcessor Specification v1.4
MPTABLE: OEM ID:  MPTABLE: Product ID:  MPTABLE: APIC at: 0xFEE00000
Processor #0 (Bootup-CPU)
I/O APIC #1 at 0xFEC00000.
Setting APIC routing to flat
Processors: 1
Allocating PCI resources starting at 10000000 (gap: 8000000:f8000000)
Built 1 zonelists.  Total pages: 30458
Kernel command line: earlyprintk=ttyS0 console=ttyS0 lpj=7999923 root=/dev/hda1
Initializing CPU#0
PID hash table entries: 512 (order: 9, 4096 bytes)
time.c: Detected 1999.998 MHz processor.
Console: colour dummy device 80x25
console handover: boot [earlyser0] -> real [ttyS0]
Dentry cache hash table entries: 16384 (order: 5, 131072 bytes)
Inode-cache hash table entries: 8192 (order: 4, 65536 bytes)
Checking aperture...
Memory: 121556k/131072k available (3742k kernel code, 8456k reserved, 1874k data, 232k init)
Calibrating delay loop (skipped)... 3999.96 BogoMIPS preset
Mount-cache hash table entries: 256
CPU: L1 I Cache: 64K (64 bytes/line), D cache 64K (64 bytes/line)
CPU: L2 Cache: 1024K (64 bytes/line)
CPU: Fake M5 x86_64 CPU stepping 01
ACPI: Core revision 20070126
ACPI Exception (tbxface-0618): AE_NO_ACPI_TABLES, While loading namespace from ACPI tables [20070126]
ACPI: Unable to load the System Description Tables
Using local APIC timer interrupts.
result 7812490
Detected 7.812 MHz APIC timer.
NET: Registered protocol family 16
PCI: Using configuration type 1
ACPI: Interpreter disabled.
Linux Plug and Play Support v0.97 (c) Adam Belay
pnp: PnP ACPI: disabled
SCSI subsystem initialized
usbcore: registered new interface driver usbfs
usbcore: registered new interface driver hub
usbcore: registered new device driver usb
PCI: Probing PCI hardware
PCI-GART: No AMD northbridge found.
NET: Registered protocol family 2
Time: tsc clocksource has been installed.
IP route cache hash table entries: 1024 (order: 1, 8192 bytes)
TCP established hash table entries: 4096 (order: 4, 65536 bytes)
TCP bind hash table entries: 4096 (order: 3, 32768 bytes)
TCP: Hash tables configured (established 4096 bind 4096)
TCP reno registered
Total HugeTLB memory allocated, 0
Installing knfsd (copyright (C) 1996 okir@monad.swb.de).
io scheduler noop registered
io scheduler deadline registered
io scheduler cfq registered (default)
Real Time Clock Driver v1.12ac
Linux agpgart interface v0.102 (c) Dave Jones
Serial: 8250/16550 driver $Revision: 1.90 $ 4 ports, IRQ sharing disabled
serial8250: ttyS0 at I/O 0x3f8 (irq = 4) is a 8250
floppy0: no floppy controllers found
RAMDISK driver initialized: 16 RAM disks of 4096K size 1024 blocksize
loop: module loaded
Intel(R) PRO/1000 Network Driver - version 7.3.20-k2
Copyright (c) 1999-2006 Intel Corporation.
e100: Intel(R) PRO/100 Network Driver, 3.5.17-k4-NAPI
e100: Copyright(c) 1999-2006 Intel Corporation
forcedeth.c: Reverse Engineered nForce ethernet driver. Version 0.60.
tun: Universal TUN/TAP device driver, 1.6
tun: (C) 1999-2004 Max Krasnyansky <maxk@qualcomm.com>
netconsole: not configured, aborting
Uniform Multi-Platform E-IDE driver Revision: 7.00alpha2
ide: Assuming 33MHz system bus speed for PIO modes; override with idebus=xx
PIIX4: IDE controller at PCI slot 0000:00:04.0
PCI: Enabling device 0000:00:04.0 (0000 -> 0001)
PIIX4: chipset revision 0
PIIX4: not 100% native mode: will probe irqs later
    ide0: BM-DMA at 0x1000-0x1007, BIOS settings: hda:DMA, hdb:DMA
    ide1: BM-DMA at 0x1008-0x100f, BIOS settings: hdc:DMA, hdd:DMA
hda: M5 IDE Disk, ATA DISK drive
hdb: M5 IDE Disk, ATA DISK drive
ide0 at 0x1f0-0x1f7,0x3f6 on irq 14
hda: max request size: 128KiB
hda: 1048320 sectors (536 MB), CHS=1040/16/63, UDMA(33)
 hda: hda1
hdb: max request size: 128KiB
hdb: 4177920 sectors (2139 MB), CHS=4144/16/63, UDMA(33)
 hdb: unknown partition table
megaraid cmm: 2.20.2.7 (Release Date: Sun Jul 16 00:01:03 EST 2006)
megaraid: 2.20.5.1 (Release Date: Thu Nov 16 15:32:35 EST 2006)
megasas: 00.00.03.10-rc5 Thu May 17 10:09:32 PDT 2007
Fusion MPT base driver 3.04.04
Copyright (c) 1999-2007 LSI Logic Corporation
Fusion MPT SPI Host driver 3.04.04
Fusion MPT SAS Host driver 3.04.04
ieee1394: raw1394: /dev/raw1394 device initialized
USB Universal Host Controller Interface driver v3.0
usbcore: registered new interface driver usblp
drivers/usb/class/usblp.c: v0.13: USB Printer Device Class driver
Initializing USB Mass Storage driver...
usbcore: registered new interface driver usb-storage
USB Mass Storage support registered.
PNP: No PS/2 controller found. Probing ports directly.
serio: i8042 KBD port at 0x60,0x64 irq 1
serio: i8042 AUX port at 0x60,0x64 irq 12
mice: PS/2 mouse device common for all mice
input: AT Translated Set 2 keyboard as /class/input/input0
device-mapper: ioctl: 4.11.0-ioctl (2006-10-12) initialised: dm-devel@redhat.com
input: PS/2 Generic Mouse as /class/input/input1
usbcore: registered new interface driver usbhid
drivers/hid/usbhid/hid-core.c: v2.6:USB HID core driver
oprofile: using timer interrupt.
TCP cubic registered
NET: Registered protocol family 1
NET: Registered protocol family 10
IPv6 over IPv4 tunneling driver
NET: Registered protocol family 17
EXT2-fs warning: mounting unchecked fs, running e2fsck is recommended
VFS: Mounted root (ext2 filesystem).
Freeing unused kernel memory: 232k freed

INIT: version 2.86 booting

mounting filesystems...
loading script...
