@ARTICLE{joukah_15,
  author={Jouppi, Norman P. and Kahng, Andrew B. and Muralimanohar, Naveen and Srinivas, Vaishnav},
  journal={IEEE Transactions on Very Large Scale Integration (VLSI) Systems}, 
  title={CACTI-IO: CACTI With OFF-Chip Power-Area-Timing Models}, 
  year={2015},
  volume={23},
  number={7},
  pages={1254-1267},
  keywords={Timing;Integrated circuit interconnections;Random access memory;Clocks;Servers;Jitter;Mobile communication;CACTI;CACTI-IO;dynamic random access memory (DRAM);IO;memory interface;power and timing models;CACTI;CACTI-IO;dynamic random access memory (DRAM);IO;memory interface;power and timing models},
  doi={10.1109/TVLSI.2014.2334635}}

@inproceedings{joukah_12,
author = {Jouppi, Norman P. and Kahng, Andrew B. and Muralimanohar, Naveen and Srinivas, Vaishnav},
title = {CACTI-IO: CACTI with off-chip power-area-timing models},
year = {2012},
isbn = {9781450315739},
publisher = {Association for Computing Machinery},
address = {New York, NY, USA},
url = {https://doi.org/10.1145/2429384.2429446},
doi = {10.1145/2429384.2429446},
booktitle = {Proceedings of the International Conference on Computer-Aided Design},
pages = {294–301},
numpages = {8},
keywords = {CACTI, DRAM, IO, memory interface, power and timing models},
location = {San Jose, California},
series = {ICCAD '12}
}

@misc{micron_ddr3_11_kopie_ipsj,
  title = {{Micron System Power Calculator}},
  author = {{Micron}},
  howpublished = {last access 2024-11-12},
  url={https://www.micron.com/sales-support/design-tools/dram-power-calculator},
  year={2014}
}

@misc{kargoo_14,
  title = {{{DRAMPower}}: {{Open-source DRAM}} Power \& Energy Estimation Tool},
  author = {Chandrasekar, Karthik and Weis, Christian and Li, Yonghui and Akesson, Benny and Naji, Omar and Jung, Matthias and Wehn, Norbert and Goossens, Kees},
  year = {Last Access 15.08.2019},
  address = {http://www.drampower.info/},
  owner = {Brugger},
  timestamp = {2019-08-15}
}

@inproceedings{junmat_16b,
  title = {A {{New Bank Sensitive DRAMPower Model}} for {{Efficient Design Space Exploration}}},
  booktitle = {International Workshop on Power and Timing Modeling, Optimization and Simulation ({{PATMOS}} 2016)},
  author = {Jung, Matthias and Mathew, Deepak M. and Zulian, {\'E}der F. and Weis, Christian and Wehn, Norbert},
  year = {2016},
  owner = {MJ},
  timestamp = {2017-06-15}
}

@inproceedings{matzul_17,
author = {Mathew, Deepak M. and Zulian, \'{E}der F. and Kannoth, Subash and Jung, Matthias and Weis, Christian and Wehn, Norbert},
title = {A Bank-Wise DRAM Power Model for System Simulations},
year = {2017},
isbn = {9781450348409},
publisher = {Association for Computing Machinery},
address = {New York, NY, USA},
url = {https://doi.org/10.1145/3023973.3023978},
doi = {10.1145/3023973.3023978},
booktitle = {Proceedings of the 9th Workshop on Rapid Simulation and Performance Evaluation: Methods and Tools},
articleno = {5},
numpages = {7},
keywords = {DRAM, Power, Simulation},
location = {Stockholm, Sweden},
series = {RAPIDO '17}
}

@article{ghoyag_18,
  title = {What {{Your DRAM Power Models Are Not Telling You}}: {{Lessons}} from a {{Detailed Experimental Study}}},
  shorttitle = {What {{Your DRAM Power Models Are Not Telling You}}},
  author = {Ghose, Saugata and Yaglik{\c c}i, Abdullah Giray and Gupta, Raghav and Lee, Donghyuk and Kudrolli, Kais and Liu, William X. and Hassan, Hasan and Chang, Kevin K. and Chatterjee, Niladrish and Agrawal, Aditya and O'Connor, Mike and Mutlu, Onur},
  year = {2018},
  month = dec,
  journal = {Proc. ACM Meas. Anal. Comput. Syst.},
  volume = {2},
  number = {3},
  pages = {38:1--38:41},
  doi = {10.1145/3224419},
  urldate = {2024-10-25},
  file = {/Users/myzinsky/Zotero/storage/NYBYGMFT/Ghose et al. - 2018 - What Your DRAM Power Models Are Not Telling You Lessons from a Detailed Experimental Study.pdf}
}

@ARTICLE{holsta_19,
  author={Hollis, Timothy M. and Stave, Eric and Ovard, Dave and Greeff, Roy and Spirkl, Worfgang and Brox, Martin and Taylor, Jennifer and Butterfield, Justin},
  journal={IEEE Solid-State Circuits Magazine}, 
  title={Recent Evolution in the DRAM Interface: Mile-Markers Along Memory Lane}, 
  year={2019},
  volume={11},
  number={2},
  pages={14-30},
  keywords={Random access memory;Bandwidth;DRAM chips;Graphics;Memory management;Semiconductor devices},
  doi={10.1109/MSSC.2019.2910617}}

@article{balkah_17,
author = {Balasubramonian, Rajeev and Kahng, Andrew B. and Muralimanohar, Naveen and Shafiee, Ali and Srinivas, Vaishnav},
title = {CACTI 7: New Tools for Interconnect Exploration in Innovative Off-Chip Memories},
year = {2017},
issue_date = {June 2017},
publisher = {Association for Computing Machinery},
address = {New York, NY, USA},
volume = {14},
number = {2},
issn = {1544-3566},
url = {https://doi.org/10.1145/3085572},
doi = {10.1145/3085572},
journal = {ACM Trans. Archit. Code Optim.},
month = jun,
articleno = {14},
numpages = {25},
keywords = {DRAM, Memory, NVM, interconnects, tools}
}

@ARTICLE{donxu_12,
  author={Dong, Xiangyu and Xu, Cong and Xie, Yuan and Jouppi, Norman P.},
  journal={IEEE Transactions on Computer-Aided Design of Integrated Circuits and Systems}, 
  title={NVSim: A Circuit-Level Performance, Energy, and Area Model for Emerging Nonvolatile Memory}, 
  year={2012},
  volume={31},
  number={7},
  pages={994-1007},
  keywords={Nonvolatile memory;Arrays;Phase change random access memory;Wires;Distributed databases;Integrated circuit modeling;Analytical circuit model;MRAM;NAND Flash;nonvolatile memory;phase-change random-access memory (PCRAM);resistive random-access memory (ReRAM);spin-torque-transfer memory (STT-RAM)},
  doi={10.1109/TCAD.2012.2185930}}

@book{dalpou_98, 
place={Cambridge}, 
title={Digital Systems Engineering}, 
publisher={Cambridge University Press}, 
author={Dally, William J. and Poulton, John W.}, 
year={1998}
}

@book{bak_90,
  title={Circuits, Interconnections, and Packaging for VLSI},
  author={Bakoglu, H.B.},
  isbn={9780201060089},
  lccn={87022964},
  series={Addison-Wesley VLSI systems series},
  year={1990},
  publisher={Addison-Wesley Publishing Company}
}

@article{10.1145/3296957.3173177,
author = {Boroumand, Amirali and Ghose, Saugata and Kim, Youngsok and Ausavarungnirun, Rachata and Shiu, Eric and Thakur, Rahul and Kim, Daehyun and Kuusela, Aki and Knies, Allan and Ranganathan, Parthasarathy and Mutlu, Onur},
title = {Google Workloads for Consumer Devices: Mitigating Data Movement Bottlenecks},
year = {2018},
issue_date = {February 2018},
publisher = {Association for Computing Machinery},
address = {New York, NY, USA},
volume = {53},
number = {2},
issn = {0362-1340},
url = {https://doi.org/10.1145/3296957.3173177},
doi = {10.1145/3296957.3173177},
abstract = {We are experiencing an explosive growth in the number of consumer devices, including smartphones, tablets, web-based computers such as Chromebooks, and wearable devices. For this class of devices, energy efficiency is a first-class concern due to the limited battery capacity and thermal power budget. We find that data movement is a major contributor to the total system energy and execution time in consumer devices. The energy and performance costs of moving data between the memory system and the compute units are significantly higher than the costs of computation. As a result, addressing data movement is crucial for consumer devices. In this work, we comprehensively analyze the energy and performance impact of data movement for several widely-used Google consumer workloads: (1) the Chrome web browser; (2) TensorFlow Mobile, Google's machine learning framework; (3) video playback, and (4) video capture, both of which are used in many video services such as YouTube and Google Hangouts. We find that processing-in-memory (PIM) can significantly reduce data movement for all of these workloads, by performing part of the computation close to memory. Each workload contains simple primitives and functions that contribute to a significant amount of the overall data movement. We investigate whether these primitives and functions are feasible to implement using PIM, given the limited area and power constraints of consumer devices. Our analysis shows that offloading these primitives to PIM logic, consisting of either simple cores or specialized accelerators, eliminates a large amount of data movement, and significantly reduces total system energy (by an average of 55.4\% across the workloads) and execution time (by an average of 54.2\%).},
journal = {SIGPLAN Not.},
month = mar,
pages = {316–331},
numpages = {16},
keywords = {consumer workloads, data movement, energy efficiency, memory systems, processing-in-memory}
}

@inproceedings{borgho_18,
author = {Boroumand, Amirali and Ghose, Saugata and Kim, Youngsok and Ausavarungnirun, Rachata and Shiu, Eric and Thakur, Rahul and Kim, Daehyun and Kuusela, Aki and Knies, Allan and Ranganathan, Parthasarathy and Mutlu, Onur},
title = {Google Workloads for Consumer Devices: Mitigating Data Movement Bottlenecks},
year = {2018},
isbn = {9781450349116},
publisher = {Association for Computing Machinery},
address = {New York, NY, USA},
url = {https://doi.org/10.1145/3173162.3173177},
doi = {10.1145/3173162.3173177},
booktitle = {Proceedings of the Twenty-Third International Conference on Architectural Support for Programming Languages and Operating Systems},
pages = {316–331},
numpages = {16},
keywords = {consumer workloads, data movement, energy efficiency, memory systems, processing-in-memory},
location = {Williamsburg, VA, USA},
series = {ASPLOS '18}
}


@inproceedings{feldmann_23,
	location = {Alexandria {VA} {USA}},
	title = {A Precise Measurement Platform for {LPDDR}4 Memories},
	isbn = {9798400716447},
	url = {https://dl.acm.org/doi/10.1145/3631882.3631899},
	doi = {10.1145/3631882.3631899},
	eventtitle = {{MEMSYS} '23: The International Symposium on Memory Systems},
	pages = {1--8},
	booktitle = {Proceedings of the International Symposium on Memory Systems},
	publisher = {{ACM}},
	author = {Feldmann, Johannes and Steiner, Lukas and Christ, Derek and Psota, Thomas and Jung, Matthias and Wehn, Norbert},
	urldate = {2024-11-14},
	date = {2023-10-02},
	langid = {english},
	file = {Feldmann et al. - 2023 - A Precise Measurement Platform for LPDDR4 Memories.pdf:/home/derek/.local/share/zotero/storage/C7RSPK9K/Feldmann et al. - 2023 - A Precise Measurement Platform for LPDDR4 Memories.pdf:application/pdf},
}

@inproceedings{vog_10,
  title = {Understanding the {{Energy Consumption}} of {{Dynamic Random Access Memories}}},
  booktitle = {2010 43rd {{Annual IEEE}}/{{ACM International Symposium}} on {{Microarchitecture}}},
  author = {Vogelsang, Thomas},
  year = {2010},
  month = dec,
  pages = {363--374},
  issn = {2379-3155},
  doi = {10.1109/MICRO.2010.42},
  urldate = {2024-11-14},
  abstract = {Energy consumption has become a major constraint on the capabilities of computer systems. In large systems the energy consumed by Dynamic Random Access Memories (DRAM) is a significant part of the total energy consumption. It is possible to calculate the energy consumption of currently available DRAMs from their datasheets, but datasheets don't allow extrapolation to future DRAM technologies and don't show how other changes like increasing bandwidth requirements change DRAM energy consumption. This paper first presents a flexible DRAM power model which uses a description of DRAM architecture, technology and operation to calculate power usage and verifies it against datasheet values. Then the model is used together with assumptions about the DRAM roadmap to extrapolate DRAM energy consumption to future DRAM generations. Using this model we evaluate some of the proposed DRAM power reduction schemes.},
  keywords = {Arrays,Capacitance,DRAM,Driver circuits,Logic gates,power,Random access memory,Transistors},
  file = {/Users/myzinsky/Zotero/storage/3LW3ARUS/Vogelsang - 2010 - Understanding the Energy Consumption of Dynamic Random Access Memories.pdf;/Users/myzinsky/Zotero/storage/HEEPHYEU/5695550.html}
}
