// -*- mode:c++ -*-

// Copyright (c) 2007 MIPS Technologies, Inc.
// All rights reserved.
//
// Redistribution and use in source and binary forms, with or without
// modification, are permitted provided that the following conditions are
// met: redistributions of source code must retain the above copyright
// notice, this list of conditions and the following disclaimer;
// redistributions in binary form must reproduce the above copyright
// notice, this list of conditions and the following disclaimer in the
// documentation and/or other materials provided with the distribution;
// neither the name of the copyright holders nor the names of its
// contributors may be used to endorse or promote products derived from
// this software without specific prior written permission.
//
// THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS
// "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT
// LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR
// A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT
// OWNER OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL,
// SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT
// LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE,
// DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY
// THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
// (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE
// OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
//
// Authors: Korey Sewell

////////////////////////////////////////////////////////////////////
//
// Base class for MIPS instructions, and some support functions
//

//Outputs to decoder.hh
output header {{

    using namespace MipsISA;

    /**
     * Base class for all MIPS static instructions.
     */
    class MipsStaticInst : public StaticInst
    {
      protected:

        // Constructor
        MipsStaticInst(const char *mnem, MachInst _machInst, OpClass __opClass)
            : StaticInst(mnem, _machInst, __opClass)
        {
        }

        /// Print a register name for disassembly given the unique
        /// dependence tag number (FP or int).
        void printReg(std::ostream &os, int reg) const;

        std::string generateDisassembly(Addr pc, const SymbolTable *symtab) const;

      public:
        void
        advancePC(MipsISA::PCState &pc) const
        {
            pc.advance();
        }
    };

}};

//Ouputs to decoder.cc
output decoder {{

    void MipsStaticInst::printReg(std::ostream &os, int reg) const
    {
        if (reg < FP_Base_DepTag) {
            ccprintf(os, "r%d", reg);
        }
        else {
            ccprintf(os, "f%d", reg - FP_Base_DepTag);
        }
    }

    std::string MipsStaticInst::generateDisassembly(Addr pc, const SymbolTable *symtab) const
    {
        std::stringstream ss;

        ccprintf(ss, "%-10s ", mnemonic);

        // Need to find standard way to not print
        // this info. Maybe add bool variable to
        // class?
        if (strcmp(mnemonic, "syscall") != 0) {
            if(_numDestRegs > 0){
                printReg(ss, _destRegIdx[0]);
            }

            if(_numSrcRegs > 0) {
                ss << ", ";
                printReg(ss, _srcRegIdx[0]);
            }

            if(_numSrcRegs > 1) {
                ss << ", ";
                printReg(ss, _srcRegIdx[1]);
            }
        }

        // Should we define a separate inst. class
        // just for two insts?
        if (strcmp(mnemonic, "sll") == 0 || strcmp(mnemonic, "sra") == 0) {
            ccprintf(ss,", %d",SA);
        }

        return ss.str();
    }

}};

